(kicad_pcb (version 20171130) (host pcbnew 5.0.2+dfsg1-1)
  (general
    (thickness 1.6)
    (drawings 37)
    (tracks 374)
    (zones 0)
    (modules 95)
    (nets 52)
  )
  (page A3)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.6)
    (trace_clearance 0.5)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.6)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5.5 5.5)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C4-Pad1)")
  (net 5 "Net-(C10-Pad1)")
  (net 6 "Net-(C12-Pad1)")
  (net 7 "Net-(C14-Pad1)")
  (net 8 "Net-(C16-Pad1)")
  (net 9 "Net-(C17-Pad1)")
  (net 10 "Net-(C17-Pad2)")
  (net 11 "Net-(C22-Pad1)")
  (net 12 "Net-(C23-Pad2)")
  (net 13 "Net-(C26-Pad1)")
  (net 14 "Net-(C27-Pad1)")
  (net 15 C+)
  (net 16 D+)
  (net 17 G+)
  (net 18 E+)
  (net 19 F+)
  (net 20 +VSW)
  (net 21 -VSW)
  (net 22 "Net-(J2-Pad1)")
  (net 23 "Net-(J10-Pad1)")
  (net 24 "Net-(J15-Pad1)")
  (net 25 "Net-(J16-Pad1)")
  (net 26 "Net-(J26-Pad1)")
  (net 27 Earth)
  (net 28 /LD_OUT)
  (net 29 "Net-(K2-Pad22)")
  (net 30 "Net-(R5-Pad1)")
  (net 31 "Net-(R18-Pad1)")
  (net 32 "Net-(R20-Pad1)")
  (net 33 "Net-(R21-Pad1)")
  (net 34 "Net-(R32-Pad2)")
  (net 35 "Net-(R34-Pad2)")
  (net 36 /HT3)
  (net 37 /HT4)
  (net 38 /HT5)
  (net 39 /HT2)
  (net 40 /HT6)
  (net 41 /HT9)
  (net 42 /HT8)
  (net 43 /HT1)
  (net 44 /MT1)
  (net 45 /MT2)
  (net 46 /MT3)
  (net 47 /MT4)
  (net 48 /HT7)
  (net 49 /CL_OUT)
  (net 50 "Net-(K1-Pad12)")
  (net 51 "Net-(D1-Pad2)")
  (net_class Default "Ceci est la Netclass par défaut."
    (clearance 0.5)
    (trace_width 0.6)
    (via_dia 0.8)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +VSW)
    (add_net -VSW)
    (add_net /CL_OUT)
    (add_net /LD_OUT)
    (add_net Earth)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C17-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C22-Pad1)")
    (add_net "Net-(C23-Pad2)")
    (add_net "Net-(C26-Pad1)")
    (add_net "Net-(C27-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J10-Pad1)")
    (add_net "Net-(J15-Pad1)")
    (add_net "Net-(J16-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J26-Pad1)")
    (add_net "Net-(K1-Pad12)")
    (add_net "Net-(K2-Pad22)")
    (add_net "Net-(R18-Pad1)")
    (add_net "Net-(R20-Pad1)")
    (add_net "Net-(R21-Pad1)")
    (add_net "Net-(R32-Pad2)")
    (add_net "Net-(R34-Pad2)")
    (add_net "Net-(R5-Pad1)")
  )
  (net_class GND ""
    (clearance 0.5)
    (trace_width 2)
    (via_dia 0.8)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (net_class HT ""
    (clearance 1.5)
    (trace_width 0.6)
    (via_dia 0.8)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /HT1)
    (add_net /HT2)
    (add_net /HT3)
    (add_net /HT4)
    (add_net /HT5)
    (add_net /HT6)
    (add_net /HT7)
    (add_net /HT8)
    (add_net /HT9)
    (add_net C+)
    (add_net D+)
    (add_net E+)
    (add_net F+)
    (add_net G+)
  )
  (net_class MT ""
    (clearance 0.8)
    (trace_width 0.6)
    (via_dia 0.8)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /MT1)
    (add_net /MT2)
    (add_net /MT3)
    (add_net /MT4)
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CB8DB01)
    (at 225 105)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.CrtYd))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (clearance 2))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CB8DB01)
    (at 295 180)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.CrtYd))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (clearance 2))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CB8DB01)
    (at 325 125)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.CrtYd))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (clearance 2))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CB8DB01)
    (at 30 120)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.CrtYd))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (clearance 2))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CB8DB01)
    (at 365 110)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.CrtYd))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (clearance 2))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CB8DB01)
    (at 165 70)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.CrtYd))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (clearance 2))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CB8DB01)
    (at 115 140)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.CrtYd))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (clearance 2))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CB8DB01)
    (at 255 155)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.CrtYd))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (clearance 2))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CB8DB01)
    (at 235 180)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.CrtYd))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (clearance 2))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CB8DB01)
    (at 125 175)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.CrtYd))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (clearance 2))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CB8DB01)
    (at 30 70)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.CrtYd))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (clearance 2))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CB8DB01)
    (at 30 165)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.CrtYd))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (clearance 2))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5CB8DB01)
    (at 325 70)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.CrtYd))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask)
      (clearance 2))
  )
  (module Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 267.335 73.9394)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D1 (at 3.81 -2.47) (layer F.SilkS))
    (fp_text value D (at 3.81 2.47) (layer F.Fab))
    (fp_text user %R (at 4.2 0) (layer F.Fab))
    (fp_text user K (at 0 -2.1) (layer F.Fab))
    (fp_text user K (at 0 -2.1) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 20 +VSW))
    (pad 2 thru_hole oval (at 7.62 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 51 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 303.657 73.6346)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D3 (at 3.81 -2.47) (layer F.SilkS))
    (fp_text value D (at 3.81 2.47) (layer F.Fab))
    (fp_text user K (at 0 -2.1) (layer F.SilkS))
    (fp_text user K (at 0 -2.1) (layer F.Fab))
    (fp_text user %R (at 4.2 0) (layer F.Fab))
    (pad 2 thru_hole oval (at 7.62 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 21 -VSW))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 20 +VSW))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57BE120D)
    (at 317.0936 90.2716)
    (descr Turret)
    (tags DEV)
    (fp_text reference J17 (at 0 -4.5) (layer F.SilkS))
    (fp_text value "CR FAT" (at 6.096 0.0508) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 45 /MT2) (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57BE120D)
    (at 317.0936 99.9236)
    (descr Turret)
    (tags DEV)
    (fp_text reference J18 (at 0 -4.5) (layer F.SilkS))
    (fp_text value "LD FAT" (at 6.0198 0.1778) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 46 /MT3) (clearance 0.5))
  )
  (module Relay_THT:Relay_DPDT_Finder_30.22 (layer F.Cu) (tedit 5A6F8F81)
    (at 303.657 77.5716 270)
    (descr "Finder 32.21-x000 Relay, DPDT, https://gfinder.findernet.com/public/attachments/30/EN/S30EN.pdf")
    (tags "AXICOM IM-Series Relay SPDT")
    (fp_text reference K3 (at 9.3 -9.9 270) (layer F.SilkS))
    (fp_text value FINDER-30.22 (at 8.4 2.4 270) (layer F.Fab))
    (fp_text user %R (at 10.2 -4.1 90) (layer F.Fab))
    (pad 21 thru_hole circle (at 7.62 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 /MT4))
    (pad 22 thru_hole circle (at 12.7 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 /MT2))
    (pad 24 thru_hole circle (at 17.78 -7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 /MT3))
    (pad A1 thru_hole rect (at 0 0) (size 1.6 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 +VSW))
    (pad A2 thru_hole circle (at 0 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 -VSW))
    (pad 11 thru_hole circle (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /LD_OUT))
    (pad 14 thru_hole circle (at 17.78 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(J16-Pad1)"))
    (pad 12 thru_hole circle (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(J15-Pad1)"))
    (model ${KISYS3DMOD}/Relay_THT.3dshapes/Relay_DPDT_Finder_30.22.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57BE120D)
    (at 317.0936 80.5942)
    (descr Turret)
    (tags DEV)
    (fp_text reference J20 (at 0 -4.5) (layer F.SilkS))
    (fp_text value FAT (at 4.7498 0.0254) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 47 /MT4) (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57BE120D)
    (at 297.7642 90.2716)
    (descr Turret)
    (tags DEV)
    (fp_text reference J15 (at 0 -4.5) (layer F.SilkS))
    (fp_text value "CR VOL" (at -6.1468 -0.0762) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(J15-Pad1)") (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57BE120D)
    (at 297.7388 99.822)
    (descr Turret)
    (tags DEV)
    (fp_text reference J16 (at 0 -4.5) (layer F.SilkS))
    (fp_text value "LD VOL" (at -6.0198 0.0508) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(J16-Pad1)") (clearance 0.5))
  )
  (module Relay_THT:Relay_DPDT_Finder_30.22 (layer F.Cu) (tedit 5A6F8F81)
    (at 267.335 77.5716 270)
    (descr "Finder 32.21-x000 Relay, DPDT, https://gfinder.findernet.com/public/attachments/30/EN/S30EN.pdf")
    (tags "AXICOM IM-Series Relay SPDT")
    (fp_text reference K1 (at 9.3 -9.9 270) (layer F.SilkS))
    (fp_text value FINDER-30.22 (at 8.4 2.4 270) (layer F.Fab))
    (fp_text user %R (at 10.2 -4.1 90) (layer F.Fab))
    (pad 12 thru_hole circle (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(K1-Pad12)"))
    (pad 14 thru_hole circle (at 17.78 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad 11 thru_hole circle (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad A2 thru_hole circle (at 0 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(D1-Pad2)"))
    (pad A1 thru_hole rect (at 0 0) (size 1.6 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 +VSW))
    (pad 24 thru_hole circle (at 17.78 -7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /LD_OUT))
    (pad 22 thru_hole circle (at 12.7 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /CL_OUT))
    (pad 21 thru_hole circle (at 7.62 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(J2-Pad1)"))
    (model ${KISYS3DMOD}/Relay_THT.3dshapes/Relay_DPDT_Finder_30.22.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57BE120D)
    (at 280.8732 85.1408)
    (descr Turret)
    (tags DEV)
    (fp_text reference J2 (at 0 -4.5) (layer F.SilkS))
    (fp_text value SEND (at 5.588 0.2286) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(J2-Pad1)") (clearance 0.5))
  )
  (module A-wai_Turrets:TUBE_PENTODE (layer F.Cu) (tedit 5CB61A11)
    (at 150 90)
    (descr Pentode)
    (fp_text reference U6 (at -10 -17.5) (layer F.SilkS))
    (fp_text value EL34 (at -10 -15) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 0 0) (size 30 30) (drill 30) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole circle (at 13.5 13.5) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (clearance 1.5))
    (pad 5 thru_hole circle (at -13.5 13.5) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C26-Pad1)") (clearance 0.5))
    (pad 8 thru_hole circle (at 0 -19) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
  )
  (module A-wai_Turrets:TUBE_TRIODE (layer F.Cu) (tedit 5CB4AC58)
    (at 80 150)
    (descr Triode)
    (fp_text reference U5 (at -14.3918 -13.729) (layer F.SilkS))
    (fp_text value ECC83 (at -14.2902 -12.0018) (layer F.SilkS))
    (pad 2 thru_hole circle (at -19 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C22-Pad1)") (clearance 0.5))
    (pad 8 thru_hole circle (at 15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(R34-Pad2)") (clearance 0.5))
    (pad "" np_thru_hole circle (at 0 0) (size 30 30) (drill 30) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 41 /HT9))
    (pad 6 thru_hole circle (at 15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 42 /HT8))
    (pad 7 thru_hole circle (at 19 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C17-Pad1)"))
  )
  (module A-wai_Turrets:TUBE_TRIODE (layer F.Cu) (tedit 57BDF36F)
    (at 225 150)
    (descr Triode)
    (fp_text reference U3 (at 11.4232 13.7284) (layer F.SilkS))
    (fp_text value ECC83 (at 11.8042 15.3032) (layer F.SilkS))
    (pad 7 thru_hole circle (at 19 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(K2-Pad22)"))
    (pad 6 thru_hole circle (at 15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 38 /HT5))
    (pad 1 thru_hole circle (at -15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 40 /HT6))
    (pad "" np_thru_hole circle (at 0 0) (size 30 30) (drill 30) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole circle (at 15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C10-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at -19 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(R18-Pad1)") (clearance 0.5))
    (pad 3 thru_hole circle (at -15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(R21-Pad1)") (clearance 0.5))
  )
  (module A-wai_Turrets:C_6PS_202 (layer F.Cu) (tedit 5CA7D1DE)
    (at 266.0904 179.8828 180)
    (descr "SBE 225P 47nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C6 (at 3.2258 1.9558 180) (layer F.SilkS))
    (fp_text value 2.2n (at -2.8702 2.1082 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -8 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.5))
    (pad 2 thru_hole circle (at 8 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C4-Pad1)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 5CC31033)
    (at 380 180)
    (descr Turret)
    (tags DEV)
    (fp_text reference J27 (at 0 -4.5) (layer F.SilkS))
    (fp_text value EARTH (at -0.0414 4.0484) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 27 Earth) (clearance 0.5))
  )
  (module Jumper:SolderJumper-2_P1.3mm_Bridged_Pad1.0x1.5mm (layer F.Cu) (tedit 5B391424)
    (at 374.7262 179.9844 180)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, bridged with 1 copper strip")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 0 -1.8 180) (layer F.SilkS))
    (fp_text value Jumper (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd custom (at -0.65 0 180) (size 1 1.5) (layers F.Cu F.Mask)
      (net 27 Earth)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy 0.4 -0.3) (xy 0.9 -0.3) (xy 0.9 0.3) (xy 0.4 0.3)) (width 0))
      ))
    (pad 2 smd rect (at 0.65 0 180) (size 1 1.5) (layers F.Cu F.Mask)
      (net 2 GND))
  )
  (module A-wai_Turrets:C_WMF_102_630V (layer F.Cu) (tedit 5CA7CF52)
    (at 199.4662 181.1528)
    (descr "M150 1µF / 100V")
    (autoplace_cost180 10)
    (fp_text reference C15 (at -3.683 -1.0414) (layer F.SilkS))
    (fp_text value 1n (at 4.0894 -1.1176) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C14-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 9.5 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:TUBE_TRIODE (layer F.Cu) (tedit 5CB4C9AB)
    (at 150 150)
    (descr Triode)
    (fp_text reference U4 (at 11.925 13.8808) (layer F.SilkS))
    (fp_text value ECC83 (at 12.0266 15.4302) (layer F.SilkS))
    (pad 3 thru_hole circle (at -15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 44 /MT1))
    (pad 8 thru_hole circle (at 15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C16-Pad1)") (clearance 0.5))
    (pad "" np_thru_hole circle (at 0 0) (size 30 30) (drill 30) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 D+))
    (pad 6 thru_hole circle (at 15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 48 /HT7))
    (pad 7 thru_hole circle (at 19 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(K1-Pad12)"))
  )
  (module A-wai_Turrets:TUBE_TRIODE (layer F.Cu) (tedit 5CB4AC19)
    (at 355 150)
    (descr Triode)
    (fp_text reference U1 (at 11.4712 13.1696) (layer F.SilkS))
    (fp_text value ECC83 (at 11.7252 14.6936) (layer F.SilkS))
    (pad 6 thru_hole circle (at 15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 43 /HT1))
    (pad 1 thru_hole circle (at -15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 39 /HT2))
    (pad "" np_thru_hole circle (at 0 0) (size 30 30) (drill 30) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole circle (at 15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(R5-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at -19 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.5))
    (pad 3 thru_hole circle (at -15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(R20-Pad1)") (clearance 0.5))
  )
  (module A-wai_Turrets:TUBE_TRIODE (layer F.Cu) (tedit 5CB4AC36)
    (at 290 150)
    (descr Triode)
    (fp_text reference U2 (at 11.625 13.2458) (layer F.SilkS))
    (fp_text value ECC83 (at 11.7774 14.846) (layer F.SilkS))
    (pad 3 thru_hole circle (at -15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)") (clearance 0.5))
    (pad 8 thru_hole circle (at 15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)") (clearance 0.5))
    (pad "" np_thru_hole circle (at 0 0) (size 30 30) (drill 30) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 37 /HT4))
    (pad 6 thru_hole circle (at 15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 36 /HT3))
  )
  (module A-wai_Turrets:C_M150_684_100V (layer F.Cu) (tedit 57E564B9)
    (at 296.3672 181.0258 180)
    (descr "M150 680nF / 100V")
    (autoplace_cost180 10)
    (fp_text reference C1 (at 6.5786 1.2446 180) (layer F.SilkS))
    (fp_text value 0.68µ (at -5.4102 1.27 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -12.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 12.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_M150_105_100V (layer F.Cu) (tedit 57E564B1)
    (at 261.587 151.511 270)
    (descr "M150 1µF / 100V")
    (autoplace_cost180 10)
    (fp_text reference C2 (at 3.81 1.237 270) (layer F.SilkS))
    (fp_text value 1µ (at -4.5212 1.2878 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 12.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (pad 1 thru_hole circle (at -12.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_6PS_502 (layer F.Cu) (tedit 5CB4C974)
    (at 313.7586 139.1158 90)
    (descr "SBE 225P 47nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C3 (at 0 -1 90) (layer F.SilkS))
    (fp_text value 4.7n (at 0 1 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -8 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.5))
    (pad 2 thru_hole circle (at 8 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 36 /HT3))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_WMF_223_630V (layer F.Cu) (tedit 5CB4B6EB)
    (at 252.824 157.1752 90)
    (descr "M150 1µF / 100V")
    (autoplace_cost180 10)
    (fp_text reference C4 (at -5.5372 -1.2116 90) (layer F.SilkS))
    (fp_text value 22n (at -5.4102 0.9474 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at 14.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 37 /HT4))
    (pad 1 thru_hole circle (at -14.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C4-Pad1)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_M150_105_100V (layer F.Cu) (tedit 57E564B1)
    (at 231.0098 181.102 180)
    (descr "M150 1µF / 100V")
    (autoplace_cost180 10)
    (fp_text reference C10 (at 6.4738 1.4986 180) (layer F.SilkS))
    (fp_text value 1µ (at 1.3938 1.4986 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -12.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C10-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 12.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_WMF_223_630V (layer F.Cu) (tedit 5CB4BA85)
    (at 225.2358 120.015)
    (descr "M150 1µF / 100V")
    (autoplace_cost180 10)
    (fp_text reference C12 (at 0 -1) (layer F.SilkS))
    (fp_text value 22n (at 0 1) (layer F.SilkS))
    (pad 1 thru_hole circle (at -14.5 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C12-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 14.5 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 38 /HT5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_6PS_503 (layer F.Cu) (tedit 5CB4B6F4)
    (at 331.5424 172.9486)
    (descr "SBE 225P 47nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C13 (at 0 -1) (layer F.SilkS))
    (fp_text value 47n (at 0 1) (layer F.SilkS))
    (pad 2 thru_hole circle (at 14 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 39 /HT2))
    (pad 1 thru_hole circle (at -14 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 49 /CL_OUT) (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_WMF_223_630V (layer F.Cu) (tedit 5CB4BA56)
    (at 186.8818 157.3022 270)
    (descr "M150 1µF / 100V")
    (autoplace_cost180 10)
    (fp_text reference C14 (at 0 -1 270) (layer F.SilkS))
    (fp_text value 22n (at 0 1 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 14.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 40 /HT6))
    (pad 1 thru_hole circle (at -14.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C14-Pad1)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_M150_105_100V (layer F.Cu) (tedit 57E564B1)
    (at 174.371 170.2816 270)
    (descr "M150 1µF / 100V")
    (autoplace_cost180 10)
    (fp_text reference C16 (at 5.3086 1.524 270) (layer F.SilkS))
    (fp_text value 1µ (at -5.5372 1.651 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -12.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C16-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 12.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_WMF_223_630V (layer F.Cu) (tedit 5CA7D089)
    (at 117.6528 144.1196 90)
    (descr "M150 1µF / 100V")
    (autoplace_cost180 10)
    (fp_text reference C17 (at -4.2418 -1.0414 90) (layer F.SilkS))
    (fp_text value 22n (at -4.191 1.016 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -14.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C17-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 14.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C17-Pad2)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_SM_500V (layer F.Cu) (tedit 5CA7D321)
    (at 47.6682 156.6776 270)
    (descr "SBE 225P 47nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C22 (at 0 -1 270) (layer F.SilkS))
    (fp_text value 500p (at 0 1 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C22-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_M150_104_630V (layer F.Cu) (tedit 5CA7D0EF)
    (at 40.7594 157.4038 270)
    (descr "M150 1µF / 100V")
    (autoplace_cost180 10)
    (fp_text reference C23 (at 0 -1 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 16 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C23-Pad2)") (clearance 0.5))
    (pad 1 thru_hole circle (at -16 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C22-Pad1)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_6PS_503 (layer F.Cu) (tedit 5CB4C9C4)
    (at 30.7086 165.4302 90)
    (descr "SBE 225P 47nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C24 (at -6.7818 -0.9398 90) (layer F.SilkS))
    (fp_text value 47n (at -6.731 1.1938 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -14 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.5))
    (pad 2 thru_hole circle (at 14 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 41 /HT9))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_6PS_503 (layer F.Cu) (tedit 5CB4C9B7)
    (at 107.1042 144.0434 90)
    (descr "SBE 225P 47nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C25 (at 0 -1 90) (layer F.SilkS))
    (fp_text value 47n (at 0 1 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -14 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.5))
    (pad 2 thru_hole circle (at 14 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 42 /HT8))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_M150_104_630V (layer F.Cu) (tedit 5CA7D0EF)
    (at 127.019 87.5284 90)
    (descr "M150 1µF / 100V")
    (autoplace_cost180 10)
    (fp_text reference C26 (at 0 -1 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -16 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C26-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 16 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_M150_104_630V (layer F.Cu) (tedit 5CA7D0EF)
    (at 56.3308 87.5538 90)
    (descr "M150 1µF / 100V")
    (autoplace_cost180 10)
    (fp_text reference C27 (at 0 -1 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -16 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C27-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 16 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:CPA_22uF_500V (layer F.Cu) (tedit 5CB4C963)
    (at 150 150 90)
    (descr "Capacitor F+T 22µF / 500V")
    (fp_text reference C29 (at 17.4882 -10.7064 90) (layer F.SilkS))
    (fp_text value 33µ (at 0 11 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at -23.7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (pad 1 thru_hole circle (at 22.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 D+))
    (model walter/capacitors/cpa_13x31mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:CPA_22uF_500V (layer F.Cu) (tedit 5CB4C978)
    (at 355 150 90)
    (descr "Capacitor F+T 22µF / 500V")
    (fp_text reference C30 (at 17.1072 -10.6268 90) (layer F.SilkS))
    (fp_text value 10µ (at 0.0892 10.7854 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 22.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 G+))
    (pad 2 thru_hole circle (at -23.7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (model walter/capacitors/cpa_13x31mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:CPA_22uF_500V (layer F.Cu) (tedit 5CB4C968)
    (at 225 150 90)
    (descr "Capacitor F+T 22µF / 500V")
    (fp_text reference C31 (at 17.3866 -10.7002 90) (layer F.SilkS))
    (fp_text value 22µ (at 0 11 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 22.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 E+))
    (pad 2 thru_hole circle (at -23.7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (model walter/capacitors/cpa_13x31mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:CPA_22uF_500V (layer F.Cu) (tedit 5CB4C96E)
    (at 290 150 90)
    (descr "Capacitor F+T 22µF / 500V")
    (fp_text reference C32 (at 17.7168 -10.7778 90) (layer F.SilkS))
    (fp_text value 10µ (at 0 11 90) (layer F.SilkS))
    (pad 2 thru_hole circle (at -23.7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (pad 1 thru_hole circle (at 22.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 F+))
    (model walter/capacitors/cpa_13x31mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_THT:D_DO-41_SOD81_P7.62mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 185.6486 82.7786)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=7.62mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 7.62mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D2 (at 3.81 -2.47) (layer F.SilkS))
    (fp_text value D (at 3.81 2.47) (layer F.Fab))
    (fp_text user %R (at 4.2 0) (layer F.Fab))
    (fp_text user K (at 0 -2.1) (layer F.Fab))
    (fp_text user K (at 0 -2.1) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 20 +VSW))
    (pad 2 thru_hole oval (at 7.62 0) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 21 -VSW))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57BE120D)
    (at 379.65 135.636)
    (descr Turret)
    (tags DEV)
    (fp_text reference J8 (at 0 -4.5) (layer F.SilkS))
    (fp_text value "CLN GND" (at 0 5) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57BE120D)
    (at 179.3494 99.5172)
    (descr Turret)
    (tags DEV)
    (fp_text reference J10 (at 0 -4.5) (layer F.SilkS))
    (fp_text value CRUNCH (at 0 5) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(J10-Pad1)") (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57BE120D)
    (at 183.3372 74.1172)
    (descr Turret)
    (tags DEV)
    (fp_text reference J14 (at 0 -4.5) (layer F.SilkS))
    (fp_text value R+ (at -4.6228 0.0508) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 20 +VSW) (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57BE120D)
    (at 194.818 74.3458)
    (descr Turret)
    (tags DEV)
    (fp_text reference J19 (at 0 -4.5) (layer F.SilkS))
    (fp_text value CR/LD (at 6.35 0.3048) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 -VSW) (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57BE120D)
    (at 31 81.1022)
    (descr Turret)
    (tags DEV)
    (fp_text reference J26 (at 0 -4.5) (layer F.SilkS))
    (fp_text value BIAS (at 0 5) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(J26-Pad1)") (clearance 0.5))
  )
  (module Relay_THT:Relay_DPDT_Finder_30.22 (layer F.Cu) (tedit 5A6F8F81)
    (at 185.6486 86.8172 270)
    (descr "Finder 32.21-x000 Relay, DPDT, https://gfinder.findernet.com/public/attachments/30/EN/S30EN.pdf")
    (tags "AXICOM IM-Series Relay SPDT")
    (fp_text reference K2 (at 9.3 -9.9 270) (layer F.SilkS))
    (fp_text value FINDER-30.22 (at 8.4 2.4 270) (layer F.Fab))
    (fp_text user %R (at 10.2 -4.1 90) (layer F.Fab))
    (pad 21 thru_hole circle (at 7.62 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 22 thru_hole circle (at 12.7 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(K2-Pad22)"))
    (pad 24 thru_hole circle (at 17.78 -7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
    (pad A1 thru_hole rect (at 0 0) (size 1.6 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 +VSW))
    (pad A2 thru_hole circle (at 0 -7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 -VSW))
    (pad 11 thru_hole circle (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(K1-Pad12)"))
    (pad 14 thru_hole circle (at 17.78 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(C14-Pad1)"))
    (pad 12 thru_hole circle (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(J10-Pad1)"))
    (model ${KISYS3DMOD}/Relay_THT.3dshapes/Relay_DPDT_Finder_30.22.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 377.0338 161.0106 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R5 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value 1.5k (at 0.127 -0.0292 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(R5-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 372.6434 122.1994)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R8 (at 0 -2.5) (layer F.SilkS))
    (fp_text value 100k (at -0.0508 0.0762) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 G+))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 43 /HT1))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 304.6654 121.7168)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R9 (at 0 -2.5) (layer F.SilkS))
    (fp_text value 120k (at -0.0686 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 F+))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 36 /HT3))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 268.1402 138.9634 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R10 (at -0.1778 2.3292 270) (layer F.SilkS))
    (fp_text value 220k (at -0.0254 0.0178 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 F+))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 37 /HT4))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 246.3178 120.1166 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R16 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value 100k (at 0.0762 -0.0368 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 38 /HT5))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 E+))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 199.658 150.0378 90)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R18 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value 470k (at 0.0254 0.1638 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(R18-Pad1)"))
    (pad 2 thru_hole circle (at 7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C12-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 199.658 164.0332 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R19 (at -0.0508 2.4778 270) (layer F.SilkS))
    (fp_text value 1M (at -0.0254 0.0394 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(R18-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 323.4398 156.9466 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R20 (at -0.1524 2.333 270) (layer F.SilkS))
    (fp_text value 4.7k (at -0.2286 -0.1054 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(R20-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 193.435 129.7686 180)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R21 (at -0.1384 2.286 180) (layer F.SilkS))
    (fp_text value 39k (at -0.0114 -0.0762 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole circle (at -7 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(R21-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 329.7136 149.987 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R22 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value 100k (at -0.1778 -0.0038 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 G+))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 39 /HT2))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 193.435 143.0528 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R23 (at -0.1524 2.2492 270) (layer F.SilkS))
    (fp_text value 100k (at -0.0508 -0.0622 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 E+))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 40 /HT6))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 332.6346 181.7116)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R24 (at -11.9088 0.0762) (layer F.SilkS))
    (fp_text value 1M (at -0.047 0.0762) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 49 /CL_OUT))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 176.7078 138.938 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R26 (at 0.2286 2.286 270) (layer F.SilkS))
    (fp_text value 2.2M (at 0.1016 -0.0508 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(K1-Pad12)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 149.9466 121.4374)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R29 (at 0 -2.5) (layer F.SilkS))
    (fp_text value 100k (at 0.0912 0.0762) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 D+))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 48 /HT7))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 5CB4C9A5)
    (at 128.1354 160.9598 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R30 (at -0.0762 2.4054 270) (layer F.SilkS))
    (fp_text value 100k (at 0 -0.0076 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 44 /MT1))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 117.6528 165.6334 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R32 (at 0.2794 2.286 270) (layer F.SilkS))
    (fp_text value 470k (at 0.1778 -0.1524 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(R32-Pad2)"))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C17-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 79.6544 128.3208)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R33 (at 0 -2.5) (layer F.SilkS))
    (fp_text value 100k (at 0.0762 0.0508) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 C+))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 42 /HT8))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 95.504 167.1828 180)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R34 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value 820R (at 0.127 -0.0762 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(R34-Pad2)"))
    (pad 1 thru_hole circle (at -7 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(R32-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 88.6206 176.1998)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R35 (at 0 -2.5) (layer F.SilkS))
    (fp_text value 22k (at -0.0508 0.0762) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(R32-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 54.6024 149.9512 90)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R36 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value 100k (at -0.0358 0.033 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 41 /HT9))
    (pad 2 thru_hole circle (at 7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 C+))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 64.4652 167.4114)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R37 (at 0 -2.5) (layer F.SilkS))
    (fp_text value 470k (at 0.127 0) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(R32-Pad2)"))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C22-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 64.6684 176.8348 180)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R38 (at 0.1524 2.3876 180) (layer F.SilkS))
    (fp_text value 470k (at -0.1016 0.0254 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole circle (at 7 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C23-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 119.2974 87.2744 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R39 (at -0.1778 2.432 270) (layer F.SilkS))
    (fp_text value 470k (at 0.0508 -0.0318 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(J26-Pad1)"))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C26-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 48.7108 87.3506 90)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R40 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value 470k (at 0.127 0.0826 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(J26-Pad1)"))
    (pad 2 thru_hole circle (at 7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C27-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_2W (layer F.Cu) (tedit 5CB4C9E4)
    (at 79.3242 119.0752 180)
    (descr "Resistance 2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R46 (at 0 -1 180) (layer F.SilkS))
    (fp_text value 2.2k/2W (at 0 1 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -8 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 D+))
    (pad 2 thru_hole circle (at 8 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 C+))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 338.7344 113.9698 180)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R47 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value 10k (at 0.0508 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 G+))
    (pad 2 thru_hole circle (at 7 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 D+))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 273.304 111.9632 180)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R49 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value 10k (at 0 0.0508 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 E+))
    (pad 1 thru_hole circle (at -7 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 F+))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:TUBE_PENTODE (layer F.Cu) (tedit 5CB61A0A)
    (at 80 90)
    (descr Pentode)
    (fp_text reference U7 (at -10 -17.5) (layer F.SilkS))
    (fp_text value EL34 (at -10 -15) (layer F.SilkS))
    (pad 8 thru_hole circle (at 0 -19) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (pad 5 thru_hole circle (at -13.5 13.5) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C27-Pad1)") (clearance 0.5))
    (pad 4 thru_hole circle (at 13.5 13.5) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (clearance 1.5))
    (pad "" np_thru_hole circle (at 0 0) (size 30 30) (drill 30) (layers *.Cu *.Mask F.SilkS))
  )
  (module A-wai_Turrets:R_2W (layer F.Cu) (tedit 5CB4C956)
    (at 38.9128 109.1184 180)
    (descr "Resistance 2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R1 (at 0 -1 180) (layer F.SilkS))
    (fp_text value 2.2k/2W (at 0 1 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -8 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 C+))
    (pad 2 thru_hole circle (at 8 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D22.0mm_P10.00mm_SnapIn (layer F.Cu) (tedit 5CB8D4C0)
    (at 54.61 123.4694 180)
    (descr "CP, Radial series, Radial, pin pitch=10.00mm, , diameter=22mm, Electrolytic Capacitor, , http://www.vishay.com/docs/28342/058059pll-si.pdf")
    (tags "CP Radial series Radial pin pitch 10.00mm  diameter 22mm Electrolytic Capacitor")
    (fp_text reference C5 (at 5 -12.25 180) (layer F.SilkS))
    (fp_text value 47µ (at 5 12.25 180) (layer F.SilkS))
    (fp_text user %R (at 5 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 15 C+))
    (pad 2 thru_hole circle (at 10 0 180) (size 4 4) (drill 2) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D22.0mm_P10.00mm_SnapIn.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 5CB8D270)
    (at 314.071 156.591)
    (descr Turret)
    (tags DEV)
    (fp_text reference J7 (at -3.81 -2.0574) (layer F.SilkS) hide)
    (fp_text value "CR GND" (at 0 5) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 5CB8E03B)
    (at 111.6838 165.7604)
    (descr Turret)
    (tags DEV)
    (fp_text reference J11 (at 0 -3.556) (layer F.SilkS))
    (fp_text value "PI GND" (at 0.0762 4.0894) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57BE120D)
    (at 48.4124 179.4302)
    (descr Turret)
    (tags DEV)
    (fp_text reference J21 (at 0 -4.5) (layer F.SilkS))
    (fp_text value "PI GND" (at 0.127 4.0086) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 176.9872 115.3414 180)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R48 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value 4.7k (at 0 -0.0254 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 E+))
    (pad 2 thru_hole circle (at 7 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 D+))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57BE120D)
    (at 280.8224 74.5236)
    (descr Turret)
    (tags DEV)
    (fp_text reference J1 (at 0 -4.5) (layer F.SilkS))
    (fp_text value CHANNEL (at 6.8072 -0.127) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(D1-Pad2)") (clearance 0.5))
  )
  (gr_line (start 28 185) (end 25 182) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 25 68) (end 28 65) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 385 182) (end 382 185) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 330 65) (end 385 120) (layer Edge.Cuts) (width 0.1))
  (gr_text LEAD (at 244.0178 154.5082) (layer F.SilkS))
  (gr_text B+ (at 30.7848 113.411) (layer F.SilkS))
  (gr_text G2 (at 163.4744 107.315) (layer F.SilkS))
  (gr_text G2 (at 93.5228 107.315) (layer F.SilkS))
  (gr_text MSTR+ (at 56.515 67.2084) (layer F.SilkS))
  (gr_text MSTR- (at 127.3302 67.1068) (layer F.SilkS))
  (gr_text RETURN (at 117.7544 124.968) (layer F.SilkS))
  (gr_text PI- (at 31.4198 183.8706) (layer F.SilkS))
  (gr_text PI+ (at 107.3404 162.4838) (layer F.SilkS))
  (gr_text "LD EQ" (at 128.143 149.5552) (layer F.SilkS))
  (gr_text "LD EQ\nGND" (at 132.08 172.339) (layer F.SilkS))
  (gr_text "LD GND" (at 283.6164 176.3522) (layer F.SilkS))
  (gr_text "LD GAIN" (at 274.0914 174.752) (layer F.SilkS))
  (gr_text "CLN VOL" (at 335.9912 154.2796) (layer F.SilkS))
  (gr_text R7 (at 263.1948 155.3718 90) (layer F.SilkS))
  (gr_text R28 (at 176.8602 175.6664 90) (layer F.SilkS))
  (gr_text R25 (at 195.8086 182.118) (layer F.SilkS))
  (gr_text R15 (at 224.4344 182.245) (layer F.SilkS))
  (gr_text 1.8k (at 263.2202 146.9136 90) (layer F.SilkS))
  (gr_text 1.8k (at 176.7586 164.7444 90) (layer F.SilkS))
  (gr_text 1.8k (at 229.8192 182.1434) (layer F.SilkS))
  (gr_text 470k (at 268.9606 181.8386) (layer F.SilkS))
  (gr_text R7 (at 263.017 181.8386) (layer F.SilkS))
  (gr_text "CLN EQ" (at 379.2982 126.5936) (layer F.SilkS))
  (gr_text "CR GAIN" (at 314.5536 151.4348) (layer F.SilkS))
  (gr_text 2.7k (at 301.5742 182.1434) (layer F.SilkS))
  (gr_text R6 (at 289.9156 182.1942) (layer F.SilkS))
  (dimension 120.015 (width 0.3) (layer Dwgs.User)
    (gr_text "120 mm" (at 398 125 270) (layer Dwgs.User))
    (feature1 (pts (xy 384.9878 185.0136) (xy 396.674021 185.0136)))
    (feature2 (pts (xy 384.9878 64.9986) (xy 396.674021 64.9986)))
    (crossbar (pts (xy 396.0876 64.9986) (xy 396.0876 185.0136)))
    (arrow1a (pts (xy 396.0876 185.0136) (xy 395.501179 183.887096)))
    (arrow1b (pts (xy 396.0876 185.0136) (xy 396.674021 183.887096)))
    (arrow2a (pts (xy 396.0876 64.9986) (xy 395.501179 66.125104)))
    (arrow2b (pts (xy 396.0876 64.9986) (xy 396.674021 66.125104)))
  )
  (dimension 359.9942 (width 0.3) (layer Dwgs.User)
    (gr_text "360 mm" (at 205 53) (layer Dwgs.User))
    (feature1 (pts (xy 384.9878 64.9986) (xy 384.9878 54.607779)))
    (feature2 (pts (xy 24.9936 64.9986) (xy 24.9936 54.607779)))
    (crossbar (pts (xy 24.9936 55.1942) (xy 384.9878 55.1942)))
    (arrow1a (pts (xy 384.9878 55.1942) (xy 383.861296 55.780621)))
    (arrow1b (pts (xy 384.9878 55.1942) (xy 383.861296 54.607779)))
    (arrow2a (pts (xy 24.9936 55.1942) (xy 26.120104 55.780621)))
    (arrow2b (pts (xy 24.9936 55.1942) (xy 26.120104 54.607779)))
  )
  (gr_line (start 25 182) (end 25 68) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 382 185) (end 28 185) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 385 120) (end 385 182) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 28 65) (end 330 65) (layer Edge.Cuts) (width 0.1))
  (zone (net 27) (net_name Earth) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 22.9362 63.2714) (xy 386.7912 62.4078) (xy 388.3406 188.4426) (xy 23.876 186.7662)
      )
    )
  )
  (zone (net 27) (net_name Earth) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 22.877366 187.144327) (xy 386.732366 188.007927) (xy 388.281766 61.973127) (xy 23.817166 63.649527)
      )
    )
  )
)
