(kicad_pcb (version 4) (host pcbnew 4.0.5+dfsg1-4)
  (general
    (links 0)
    (no_connects 0)
    (area 53.848 90.678 361.569001 231.902001)
    (thickness 1.6)
    (drawings 23)
    (tracks 275)
    (zones 0)
    (modules 71)
    (nets 42)
  )
  (page A3)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.8)
    (trace_clearance 0.8)
    (zone_clearance 0.8)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.8)
    (via_drill 0.6)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.5 3.5)
    (pad_drill 3.5)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFDF7F)
    (pcbplotparams
      (layerselection 0x010e0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerber/))
  )
  (net 0 "")
  (net 1 F+)
  (net 2 GND)
  (net 3 E+)
  (net 4 D+)
  (net 5 /HT_U2A)
  (net 6 "Net-(C8-Pad2)")
  (net 7 /HT_U2B)
  (net 8 "Net-(C11-Pad1)")
  (net 9 "Net-(C10-Pad2)")
  (net 10 /HT_U4B)
  (net 11 "Net-(C16-Pad2)")
  (net 12 /HT_U4A)
  (net 13 "Net-(C18-Pad2)")
  (net 14 "Net-(D1-Pad1)")
  (net 15 "Net-(D1-Pad2)")
  (net 16 C+)
  (net 17 "Net-(C6-Pad2)")
  (net 18 /HT_G2)
  (net 19 "Net-(C3-Pad1)")
  (net 20 "Net-(C7-Pad1)")
  (net 21 "Net-(R14-Pad2)")
  (net 22 "Net-(R16-Pad1)")
  (net 23 "Net-(C12-Pad1)")
  (net 24 /HT_U3A)
  (net 25 /HT_U3B)
  (net 26 "Net-(R31-Pad1)")
  (net 27 Earth)
  (net 28 "Net-(C21-Pad2)")
  (net 29 "Net-(P17-Pad1)")
  (net 30 "Net-(R25-Pad2)")
  (net 31 "Net-(R34-Pad1)")
  (net 32 /HT)
  (net 33 "Net-(R37-Pad1)")
  (net 34 "Net-(C10-Pad1)")
  (net 35 "Net-(K2-Pad11)")
  (net 36 "Net-(K2-Pad6)")
  (net 37 "Net-(K2-Pad4)")
  (net 38 "Net-(P16-Pad1)")
  (net 39 "Net-(P19-Pad1)")
  (net 40 "Net-(K2-Pad8)")
  (net 41 "Net-(JP2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.8)
    (trace_width 0.8)
    (via_dia 0.8)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C16-Pad2)")
    (add_net "Net-(C18-Pad2)")
    (add_net "Net-(C21-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(JP2-Pad2)")
    (add_net "Net-(K2-Pad11)")
    (add_net "Net-(K2-Pad4)")
    (add_net "Net-(K2-Pad6)")
    (add_net "Net-(K2-Pad8)")
    (add_net "Net-(P16-Pad1)")
    (add_net "Net-(P17-Pad1)")
    (add_net "Net-(P19-Pad1)")
    (add_net "Net-(R14-Pad2)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(R25-Pad2)")
    (add_net "Net-(R31-Pad1)")
    (add_net "Net-(R34-Pad1)")
    (add_net "Net-(R37-Pad1)")
  )
  (net_class GND ""
    (clearance 0.8)
    (trace_width 2)
    (via_dia 0.8)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net Earth)
    (add_net GND)
  )
  (net_class HT ""
    (clearance 1.8)
    (trace_width 0.8)
    (via_dia 0.8)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /HT)
    (add_net /HT_G2)
    (add_net /HT_U2A)
    (add_net /HT_U2B)
    (add_net /HT_U3A)
    (add_net /HT_U3B)
    (add_net /HT_U4A)
    (add_net /HT_U4B)
    (add_net C+)
    (add_net D+)
    (add_net E+)
    (add_net F+)
  )
  (module SMD_Packages:1Pin (layer F.Cu) (tedit 59188EBE)
    (at 85 216.5)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3) (layer F.SilkS) hide)
    (fp_text value 1Pin (at 0 3) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask)
      (clearance 2))
  )
  (module SMD_Packages:1Pin (layer F.Cu) (tedit 59188ED2)
    (at 185 215)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3) (layer F.SilkS) hide)
    (fp_text value 1Pin (at 0 3) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask)
      (clearance 2))
  )
  (module SMD_Packages:1Pin (layer F.Cu) (tedit 59188ECE)
    (at 290 140)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3) (layer F.SilkS) hide)
    (fp_text value 1Pin (at 0 3) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask)
      (clearance 2))
  )
  (module SMD_Packages:1Pin (layer F.Cu) (tedit 59188ECC)
    (at 210 135)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3) (layer F.SilkS) hide)
    (fp_text value 1Pin (at 0 3) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask)
      (clearance 2))
  )
  (module SMD_Packages:1Pin (layer F.Cu) (tedit 59188EC9)
    (at 180 105)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3) (layer F.SilkS) hide)
    (fp_text value 1Pin (at 0 3) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask)
      (clearance 2))
  )
  (module SMD_Packages:1Pin (layer F.Cu) (tedit 59188EC4)
    (at 75 105)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3) (layer F.SilkS) hide)
    (fp_text value 1Pin (at 0 3) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask)
      (clearance 2))
  )
  (module Diodes_SMD:SMB_Handsoldering (layer B.Cu) (tedit 59188D4F)
    (at 135.636 173.5582)
    (descr "Diode SMB Handsoldering")
    (tags "Diode SMB Handsoldering")
    (attr smd)
    (fp_text reference JP2 (at -0.1524 5.2832) (layer F.SilkS) hide)
    (fp_text value JUMPER (at 0 -4) (layer B.Fab) hide)
    (fp_text user K (at -3 -3) (layer F.SilkS) hide)
    (fp_text user A (at 3 -3) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2 0) (size 3 2) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C18-Pad2)"))
    (pad 2 smd rect (at 2 0) (size 3 2) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(JP2-Pad2)"))
    (model Diodes_SMD.3dshapes/SMB_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0 0 0))
      (rotate (xyz 0 0 180))
    )
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 591879BB)
    (at 100.8634 217.0938)
    (descr Turret)
    (tags DEV)
    (fp_text reference TURRET (at 0 -1.905) (layer F.SilkS) hide)
    (fp_text value P*** (at 0 2.032) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 27 Earth) (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 591879BB)
    (at 166.1922 169.2656)
    (descr Turret)
    (tags DEV)
    (fp_text reference TURRET (at 0 -1.905) (layer F.SilkS) hide)
    (fp_text value P*** (at 0 2.032) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 27 Earth) (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 591879BB)
    (at 154.1526 179.7812)
    (descr Turret)
    (tags DEV)
    (fp_text reference TURRET (at 0 -1.905) (layer F.SilkS) hide)
    (fp_text value P*** (at 0 2.032) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 27 Earth) (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 591879BB)
    (at 237.5916 184.8612)
    (descr Turret)
    (tags DEV)
    (fp_text reference TURRET (at 0 -1.905) (layer F.SilkS) hide)
    (fp_text value P*** (at 0 2.032) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 27 Earth) (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 591879BB)
    (at 110.4646 203.6826)
    (descr Turret)
    (tags DEV)
    (fp_text reference TURRET (at 0 -1.905) (layer F.SilkS) hide)
    (fp_text value P*** (at 0 2.032) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 27 Earth) (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 591879BB)
    (at 217.1954 213.4616)
    (descr Turret)
    (tags DEV)
    (fp_text reference TURRET (at 0 -1.905) (layer F.SilkS) hide)
    (fp_text value P*** (at 0 2.032) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 27 Earth) (clearance 0.5))
  )
  (module A-wai_Turrets:TUBE_TRIODE (layer F.Cu) (tedit 591862DC)
    (at 265 185)
    (descr Triode)
    (fp_text reference U2 (at 8.6088 -18.1728) (layer F.SilkS))
    (fp_text value ECC83 (at 8.7104 -16.6996) (layer F.SilkS))
    (pad 3 thru_hole circle (at -15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(C7-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at -19 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.5))
    (pad 8 thru_hole circle (at 15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(C3-Pad1)") (clearance 0.5))
    (pad "" np_thru_hole circle (at 0 0) (size 30 30) (drill 30) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 /HT_U2B))
    (pad 6 thru_hole circle (at 15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 /HT_U2A))
  )
  (module A-wai_Turrets:C_225P_223_400V (layer F.Cu) (tedit 57D574FA)
    (at 238.4806 209.2198 180)
    (descr "SBE 225P 22nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C8 (at 0.1016 1.1811 180) (layer F.SilkS))
    (fp_text value 22n (at 0 -0.7747 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 /HT_U2B))
    (pad 2 thru_hole circle (at 9.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C8-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57E5A34D)
    (at 294.9956 214.5792)
    (descr Turret)
    (tags DEV)
    (fp_text reference P14 (at 0 -4.5) (layer Cmts.User))
    (fp_text value EARTH (at 0.127 4.064) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 27 Earth) (clearance 0.5))
  )
  (module A-wai_Turrets:C_225P_223_400V (layer F.Cu) (tedit 57D564C1)
    (at 212.344 167.8178 270)
    (descr "SBE 225P 22nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C9 (at 0.0508 1.1176 270) (layer F.SilkS))
    (fp_text value 22n (at -0.2794 -1.1684 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 /HT_U3A) (clearance 0.5))
    (pad 2 thru_hole circle (at 9.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C11-Pad1)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_2W (layer F.Cu) (tedit 57D57142)
    (at 93.8276 107.8484)
    (descr "Resistance 2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R7 (at 0 -1) (layer F.SilkS))
    (fp_text value 10k/2W (at 0 1) (layer F.SilkS))
    (pad 1 thru_hole circle (at -8 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 C+))
    (pad 2 thru_hole circle (at 8 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 D+))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 110.3884 138.5166 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R38 (at 0.112 2.413 270) (layer F.SilkS))
    (fp_text value 470k (at 0.127 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(P16-Pad1)"))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:CPA_22uF_450V (layer F.Cu) (tedit 57D5719A)
    (at 264.9982 184.4826 90)
    (descr "Capacitor F+T 22µF / 450V")
    (fp_text reference C1 (at -14.8295 10.4775 180) (layer F.SilkS))
    (fp_text value 22µ/450V (at -17.433 9.144 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 18 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 F+))
    (pad 2 thru_hole circle (at -19.2 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (model walter/capacitors/cpa_13x31mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:CPA_47uF_450V (layer F.Cu) (tedit 57D57137)
    (at 104.2035 186.8805 90)
    (descr "Capacitor F+T 47µF / 450V")
    (fp_text reference C4 (at -19.6215 10.7315 180) (layer F.SilkS))
    (fp_text value 47µ/450V (at -22.1361 7.9121 360) (layer F.SilkS))
    (pad 1 thru_hole circle (at 22.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 D+))
    (pad 2 thru_hole circle (at -23.7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (model walter/capacitors/cpa_13x31mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Passive:DIODE (layer F.Cu) (tedit 57BE0F22)
    (at 253.3142 150.6728 90)
    (descr "Diode 1N4007")
    (tags "DIODE DEV")
    (fp_text reference D1 (at 0 2.54 90) (layer F.SilkS))
    (fp_text value 1N4007 (at 0 -2.54 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 3.81 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(D1-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(D1-Pad2)") (clearance 0.5))
    (model discret/diode.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Misc:relay-G5V2 (layer F.Cu) (tedit 57BDE8F3)
    (at 239.9284 150.622)
    (descr RELAY)
    (tags RELAY)
    (attr virtual)
    (fp_text reference K1 (at -5.08 0) (layer F.SilkS))
    (fp_text value G5V2 (at 4.064 0.127) (layer F.SilkS))
    (pad 9 thru_hole oval (at -10.16 3.81) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
    (pad 11 thru_hole oval (at -5.08 3.81) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C8-Pad2)"))
    (pad 16 thru_hole oval (at 7.62 3.81) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(D1-Pad2)"))
    (pad 1 thru_hole oval (at 7.62 -3.81) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(D1-Pad1)"))
    (pad 6 thru_hole oval (at -5.08 -3.81) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole oval (at -10.16 -3.81) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 0 -3.81) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole oval (at 0 3.81) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57E5A2DB)
    (at 181.737 146.5326)
    (descr Turret)
    (tags DEV)
    (fp_text reference P1 (at 3.556 -3.175) (layer Cmts.User))
    (fp_text value RLY+ (at 0.254 -3.7846) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(D1-Pad1)") (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57E5A2DE)
    (at 191.2874 146.5326)
    (descr Turret)
    (tags DEV)
    (fp_text reference P2 (at 0 -4.5) (layer Cmts.User))
    (fp_text value RLY- (at 0 -3.81) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(D1-Pad2)") (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57E5A328)
    (at 163.195 135.0772)
    (descr Turret)
    (tags DEV)
    (fp_text reference P6 (at 0 -4.5) (layer Cmts.User))
    (fp_text value GND (at 0 -4.3688) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57E5A4D5)
    (at 143.5608 107.442)
    (descr Turret)
    (tags DEV)
    (fp_text reference P11 (at 0 -4.5) (layer Cmts.User))
    (fp_text value Ug2 (at 0.0254 3.7338) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 /HT_G2))
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 250.7234 162.56)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R2 (at 0 -2.5) (layer F.SilkS))
    (fp_text value 10k (at -0.127 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 E+))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 F+))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 115.1232 155.0924)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R4 (at 0 -2.159) (layer F.SilkS))
    (fp_text value 10k (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 D+))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 E+))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 271.9832 158.6738)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R6 (at 0 -2.5) (layer F.SilkS))
    (fp_text value 220k (at 0.1397 0.0508) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 F+))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 /HT_U2A))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 239.7252 184.9905 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R13 (at -3.9139 -3.1115 540) (layer F.SilkS))
    (fp_text value 100k (at -0.4341 -0.1143 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 F+))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 /HT_U2B))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 226.2378 185.1406 90)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R14 (at -0.2009 -2.1082 90) (layer F.SilkS))
    (fp_text value 470k (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C8-Pad2)"))
    (pad 2 thru_hole circle (at 7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(R14-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 247.8786 204.47)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R15 (at 0 -2.5) (layer F.SilkS))
    (fp_text value 1M (at 0.254 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(R14-Pad2)"))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 207.7974 199.263 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R16 (at 0.0635 2.1717 270) (layer F.SilkS))
    (fp_text value 39k (at 0 0.127 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(R16-Pad1)"))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 206.1464 160.1216 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R18 (at -0.0762 2.4384 270) (layer F.SilkS))
    (fp_text value 100k (at -0.254 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 E+))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 /HT_U3A))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 161.5948 185.1256 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R24 (at 3.9012 -3.0226 360) (layer F.SilkS))
    (fp_text value 220k (at 0.015 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 E+))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 /HT_U3B))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 147.6502 193.548 90)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R25 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value 1M (at -0.0762 0.0254 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C16-Pad2)"))
    (pad 2 thru_hole circle (at 7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(R25-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 166.751 204.2922)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R27 (at -0.3048 -2.3876) (layer F.SilkS))
    (fp_text value 100k (at -0.097 -0.127) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(R25-Pad2)"))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 127.8128 199.4662 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R31 (at 0.0254 2.3622 270) (layer F.SilkS))
    (fp_text value 2.2k (at -0.1524 0.0254 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(R31-Pad1)"))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 119.5832 164.3126)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R32 (at 0.0762 2.3114) (layer F.SilkS))
    (fp_text value 220k (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 D+))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 /HT_U4A))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 140.1826 176.5808 90)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R34 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value 1M (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(R34-Pad1)"))
    (pad 2 thru_hole circle (at 7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(JP2-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 76.9366 176.8706 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R37 (at 0.0912 2.2098 270) (layer F.SilkS))
    (fp_text value 2.2k (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(R37-Pad1)"))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 59186487)
    (at 294.4114 184.3786)
    (descr Turret)
    (tags DEV)
    (fp_text reference P15 (at 0 -4.5) (layer Cmts.User))
    (fp_text value "LD GND" (at 0 3.683) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
  )
  (module Freetronics:SJ_OPEN (layer F.Cu) (tedit 59188F6E)
    (at 294.9956 209.8802 270)
    (descr "<b>Solder jumper</b>")
    (fp_text reference JP1 (at 0 -1.7 270) (layer F.SilkS) hide)
    (fp_text value JUMPER (at 0 1.6 270) (layer Eco1.User) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 1.1684 1.6002) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 1.1684 1.6002) (layers F.Cu F.Mask)
      (net 27 Earth))
  )
  (module A-wai_Turrets:C_225P_472_400V (layer F.Cu) (tedit 57E5649E)
    (at 288.3154 167.0308 270)
    (descr "SBE 225P 4.7nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C6 (at 4.826 1.3335 270) (layer F.SilkS))
    (fp_text value 2.2n (at -3.81 1.2065 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C10-Pad2)") (clearance 0.5))
    (pad 2 thru_hole circle (at 9.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(C6-Pad2)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_M150_105_100V (layer F.Cu) (tedit 57E564B1)
    (at 232.0925 185.0104 270)
    (descr "M150 1µF / 100V")
    (autoplace_cost180 10)
    (fp_text reference C7 (at 3.3655 0.889 270) (layer F.SilkS))
    (fp_text value 1µ (at -2.7305 1.0795 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -12.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(C7-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 12.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_225P_472_400V (layer F.Cu) (tedit 57E5649E)
    (at 218.694 191.9097 270)
    (descr "SBE 225P 4.7nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C11 (at 4.0005 1.0795 270) (layer F.SilkS))
    (fp_text value 1n (at -2.9845 1.397 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C11-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 9.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_M150_105_100V (layer F.Cu) (tedit 57E564B1)
    (at 155.194 185.0898 270)
    (descr "M150 1µF / 100V")
    (autoplace_cost180 10)
    (fp_text reference C12 (at 3.2258 0.9652 270) (layer F.SilkS))
    (fp_text value 1µ (at -2.7178 1.1684 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -12.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(C12-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 12.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_225P_223_400V (layer F.Cu) (tedit 57E56479)
    (at 157.251 209.0928 180)
    (descr "SBE 225P 22nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C16 (at 0.2286 1.0414 180) (layer F.SilkS))
    (fp_text value 22n (at -0.1524 -1.143 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 /HT_U3B) (clearance 0.5))
    (pad 2 thru_hole circle (at 9.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C16-Pad2)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_225P_223_400V (layer F.Cu) (tedit 57E56479)
    (at 133.5786 168.1988 270)
    (descr "SBE 225P 22nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C18 (at 0 -1 270) (layer F.SilkS))
    (fp_text value 22n (at 0 1 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 /HT_U4A) (clearance 0.5))
    (pad 2 thru_hole circle (at 9.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C18-Pad2)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_225P_223_400V (layer F.Cu) (tedit 57E56479)
    (at 84.2518 215.3666 180)
    (descr "SBE 225P 22nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C21 (at 4.1148 -0.1778 180) (layer F.SilkS))
    (fp_text value 22n (at -4.6482 0.0508 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 /HT_U4B) (clearance 0.5))
    (pad 2 thru_hole circle (at 9.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(C21-Pad2)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:CPA_47uF_450V (layer F.Cu) (tedit 558F0E57)
    (at 92.6338 140.1572 90)
    (descr "Capacitor F+T 47µF / 450V")
    (fp_text reference C25 (at 0 -11 90) (layer F.SilkS))
    (fp_text value 47µ/450V (at 0 11 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 22.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 C+) (clearance 0.5))
    (pad 2 thru_hole circle (at -23.7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (model walter/capacitors/cpa_13x31mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 132.1562 192.6844 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R3 (at 0.0635 -2.413 270) (layer F.SilkS))
    (fp_text value 2.2M (at 0.127 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C18-Pad2)"))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 81.4832 202.9564 90)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R35 (at 0.0508 2.3876 90) (layer F.SilkS))
    (fp_text value 1M (at -0.0254 0.0508 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(C21-Pad2)"))
    (pad 2 thru_hole circle (at 7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(R34-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 137.922 198.4756 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R36 (at -0.015 2.3368 270) (layer F.SilkS))
    (fp_text value 1M (at 0.0612 -0.0508 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(R34-Pad1)"))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 82.1436 170.6118 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R39 (at 0 -2.3114 270) (layer F.SilkS))
    (fp_text value 100k (at -0.127 -0.0508 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 D+))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 /HT_U4B))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 72.9996 197.8764 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R41 (at 0.2436 -2.2098 270) (layer F.SilkS))
    (fp_text value 330k (at 0.036776 -0.083268 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(P17-Pad1)"))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(C21-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_2W (layer F.Cu) (tedit 57BE1221)
    (at 77.1144 124.1308 90)
    (descr "Resistance 2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R45 (at 0 -1 90) (layer F.SilkS))
    (fp_text value 10k/2W (at 0 1 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -8 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 32 /HT) (clearance 0.5))
    (pad 2 thru_hole circle (at 8 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 C+) (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:TUBE_TRIODE (layer F.Cu) (tedit 58EBF438)
    (at 185 185)
    (descr Triode)
    (fp_text reference U3 (at -7.5 -17.5) (layer F.SilkS) hide)
    (fp_text value ECC83 (at -7.5 -15) (layer F.SilkS) hide)
    (pad 3 thru_hole circle (at -15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(C12-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at -19 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C11-Pad1)") (clearance 0.5))
    (pad 8 thru_hole circle (at 15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(R16-Pad1)") (clearance 0.5))
    (pad "" np_thru_hole circle (at 0 0) (size 30 30) (drill 30) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 /HT_U3B))
    (pad 6 thru_hole circle (at 15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 /HT_U3A))
    (pad 7 thru_hole circle (at 19 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(R14-Pad2)"))
  )
  (module A-wai_Turrets:TUBE_TRIODE (layer F.Cu) (tedit 58EBEF1D)
    (at 105 185)
    (descr Triode)
    (fp_text reference U4 (at -7.5 -17.5) (layer F.SilkS) hide)
    (fp_text value ECC83 (at -7.5 -15) (layer F.SilkS) hide)
    (pad 3 thru_hole circle (at -15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(R37-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at -19 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(R34-Pad1)") (clearance 0.5))
    (pad 8 thru_hole circle (at 15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(R31-Pad1)") (clearance 0.5))
    (pad "" np_thru_hole circle (at 0 0) (size 30 30) (drill 30) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 /HT_U4B))
    (pad 6 thru_hole circle (at 15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 /HT_U4A))
    (pad 7 thru_hole circle (at 19 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(R25-Pad2)"))
  )
  (module A-wai_Turrets:C_M150_105_100V (layer F.Cu) (tedit 57E564B1)
    (at 287.0962 200.8664 270)
    (descr "M150 1µF / 100V")
    (autoplace_cost180 10)
    (fp_text reference C3 (at 4.4545 2.2225 270) (layer F.SilkS))
    (fp_text value 1µ (at -4.0545 2.4765 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -12.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(C3-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 12.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_225P_223_400V (layer F.Cu) (tedit 57E56479)
    (at 282.7528 150.1648)
    (descr "SBE 225P 22nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C5 (at 0 -1) (layer F.SilkS))
    (fp_text value 22n (at 0 1) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 /HT_U2A) (clearance 0.5))
    (pad 2 thru_hole circle (at 9.5 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C10-Pad2)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:CPA_33uF_450V (layer F.Cu) (tedit 57D3C462)
    (at 185.006 184.2752 90)
    (descr "Capacitor F+T 22µF / 450V")
    (fp_text reference C2 (at -18.493 10.193 180) (layer F.SilkS))
    (fp_text value 33µ/450V (at -21.3378 10.0914 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 21.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 E+) (clearance 0.5))
    (pad 2 thru_hole circle (at -22.7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (model walter/capacitors/cpa_13x31mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_225P_472_400V (layer F.Cu) (tedit 57E5649E)
    (at 296.4434 166.9288 90)
    (descr "SBE 225P 4.7nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C10 (at -4.3434 -1.4986 90) (layer F.SilkS))
    (fp_text value 100p (at 3.4798 -1.4224 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(C10-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 9.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C10-Pad2)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Passive:DIODE (layer F.Cu) (tedit 57BE0F22)
    (at 169.3418 153.8224 90)
    (descr "Diode 1N4007")
    (tags "DIODE DEV")
    (fp_text reference D2 (at 0 2.54 90) (layer F.SilkS))
    (fp_text value 1N4007 (at 0 -2.54 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 3.81 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(D1-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at -3.81 0 90) (size 2 2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(D1-Pad2)") (clearance 0.5))
    (model discret/diode.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Misc:relay-G5V2 (layer F.Cu) (tedit 57BDE8F3)
    (at 155.8036 153.7462)
    (descr RELAY)
    (tags RELAY)
    (attr virtual)
    (fp_text reference K2 (at -5.08 0) (layer F.SilkS))
    (fp_text value G5V2 (at 4.064 0.127) (layer F.SilkS))
    (pad 9 thru_hole oval (at -10.16 3.81) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C18-Pad2)"))
    (pad 11 thru_hole oval (at -5.08 3.81) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(K2-Pad11)"))
    (pad 16 thru_hole oval (at 7.62 3.81) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(D1-Pad2)"))
    (pad 1 thru_hole oval (at 7.62 -3.81) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(D1-Pad1)"))
    (pad 6 thru_hole oval (at -5.08 -3.81) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(K2-Pad6)"))
    (pad 8 thru_hole oval (at -10.16 -3.81) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(K2-Pad8)"))
    (pad 4 thru_hole oval (at 0 -3.81) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(K2-Pad4)"))
    (pad 13 thru_hole oval (at 0 3.81) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(JP2-Pad2)"))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 591889A4)
    (at 145.7452 163.5506)
    (descr Turret)
    (tags DEV)
    (fp_text reference P9 (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value "FROM CLN" (at 0.0762 3.6068) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(K2-Pad11)") (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 5918899D)
    (at 158.3182 141.6812)
    (descr Turret)
    (tags DEV)
    (fp_text reference P10 (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value "FROM EQ" (at 0.0508 4.5466) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(K2-Pad6)") (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 591889A0)
    (at 133.3246 146.7104)
    (descr Turret)
    (tags DEV)
    (fp_text reference P12 (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value "FROM LD" (at 0 5) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(K2-Pad8)") (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 5918899B)
    (at 167.894 141.7574)
    (descr Turret)
    (tags DEV)
    (fp_text reference P13 (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value FX (at -0.0508 4.5974) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(K2-Pad4)") (clearance 0.5))
  )
  (module A-wai_Turrets:TUBE_PENTODE (layer F.Cu) (tedit 57BDF31C)
    (at 130 125)
    (descr Pentode)
    (fp_text reference U6 (at -10 -17.5) (layer F.SilkS))
    (fp_text value 6V6 (at -10 -15) (layer F.SilkS))
    (pad 3 thru_hole circle (at 0 -19) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(P19-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at -13.5 13.5) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(P16-Pad1)") (clearance 0.5))
    (pad 9 thru_hole circle (at 13.5 13.5) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 /HT_G2) (clearance 0.5))
    (pad "" np_thru_hole circle (at 0 0) (size 30 30) (drill 30) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_text "R1   1M" (at 297.6118 166.9288 90) (layer F.SilkS))
  (gr_text "FROM\nLD GAIN" (at 245.999 189.5094) (layer F.SilkS))
  (gr_text HT (at 77.089 136.9822) (layer F.SilkS))
  (gr_text "R23  1.8k" (at 156.6418 184.9374 90) (layer F.SilkS))
  (gr_text "R20   330k" (at 220.218 191.9097 90) (layer F.SilkS))
  (gr_text "R12   1.8k" (at 233.426 185.0009 90) (layer F.SilkS))
  (gr_text "R9   470k" (at 289.6362 167.0812 90) (layer F.SilkS))
  (gr_text "R5    1.8k" (at 289.5854 200.8378 90) (layer F.SilkS))
  (gr_text "Eddie Baby\nA-wai Amplification" (at 268.1478 140.8176) (layer F.SilkS))
  (gr_text EQ (at 72.9742 187.2742) (layer F.SilkS))
  (gr_text "CLN VOL" (at 296.545 179.7812) (layer F.SilkS))
  (gr_text C+ (at 77.089 111.3282) (layer F.SilkS))
  (gr_text "LD GAIN" (at 288.4424 179.7812) (layer F.SilkS))
  (gr_line (start 297 220) (end 300 217) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 70 217) (end 73 220) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 70 103) (end 73 100) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185 100) (end 220 135) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 295 135) (end 300 140) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 220 135) (end 295 135) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 70 103) (end 70 217) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185 100) (end 73 100) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 300 217) (end 300 140) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73 220) (end 297 220) (layer Edge.Cuts) (width 0.1))
  (zone (net 27) (net_name Earth) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.8))
    (min_thickness 0.5)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 354.253676 96.647) (xy 352.729676 221.996) (xy 63.804676 225.933) (xy 61.772676 96.647)
      )
    )
  )
  (zone (net 27) (net_name Earth) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.8))
    (min_thickness 0.5)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 58.674 90.678) (xy 361.569 94.615) (xy 357.124 225.298) (xy 53.848 231.902) (xy 56.515 91.313)
      )
    )
  )
)
