(kicad_pcb (version 4) (host pcbnew 4.0.7+dfsg1-1)
  (general
    (links 137)
    (no_connects 18)
    (area 69.949999 99.949999 350.050001 220.050001)
    (thickness 1.6)
    (drawings 28)
    (tracks 382)
    (zones 0)
    (modules 97)
    (nets 53)
  )
  (page A3)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.8)
    (trace_clearance 0.8)
    (zone_clearance 0.8)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.8)
    (via_drill 0.6)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.5 3.5)
    (pad_drill 3.5)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFDF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerber/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /HT_U1A)
  (net 3 "Net-(C5-Pad2)")
  (net 4 /HT_U2A)
  (net 5 "Net-(C8-Pad2)")
  (net 6 /HT_U2B)
  (net 7 "Net-(C11-Pad1)")
  (net 8 /HT_U1B)
  (net 9 "Net-(C10-Pad2)")
  (net 10 "Net-(C14-Pad1)")
  (net 11 "Net-(C14-Pad2)")
  (net 12 /HT_U4B)
  (net 13 "Net-(C16-Pad2)")
  (net 14 "Net-(C17-Pad1)")
  (net 15 /HT_U4A)
  (net 16 "Net-(C18-Pad2)")
  (net 17 "Net-(C20-Pad2)")
  (net 18 "Net-(D1-Pad1)")
  (net 19 "Net-(D1-Pad2)")
  (net 20 "Net-(C6-Pad2)")
  (net 21 /HT_G2)
  (net 22 "Net-(C3-Pad1)")
  (net 23 "Net-(C7-Pad1)")
  (net 24 "Net-(R14-Pad2)")
  (net 25 "Net-(R16-Pad1)")
  (net 26 "Net-(R17-Pad1)")
  (net 27 "Net-(C12-Pad1)")
  (net 28 /HT_U3A)
  (net 29 /HT_U3B)
  (net 30 "Net-(R31-Pad1)")
  (net 31 Earth)
  (net 32 "Net-(C13-Pad1)")
  (net 33 "Net-(C15-Pad1)")
  (net 34 "Net-(C15-Pad2)")
  (net 35 /HT_U5B)
  (net 36 "Net-(C21-Pad2)")
  (net 37 "Net-(C22-Pad1)")
  (net 38 "Net-(C23-Pad1)")
  (net 39 "Net-(P17-Pad1)")
  (net 40 "Net-(R10-Pad2)")
  (net 41 "Net-(R10-Pad1)")
  (net 42 "Net-(R25-Pad2)")
  (net 43 "Net-(R28-Pad1)")
  (net 44 "Net-(R34-Pad1)")
  (net 45 /HT)
  (net 46 "Net-(R37-Pad1)")
  (net 47 "Net-(C1-Pad1)")
  (net 48 "Net-(C2-Pad1)")
  (net 49 "Net-(C4-Pad1)")
  (net 50 "Net-(C24-Pad1)")
  (net 51 "Net-(C25-Pad1)")
  (net 52 "Net-(P10-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.8)
    (trace_width 0.8)
    (via_dia 0.8)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /HT)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C14-Pad2)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C15-Pad2)")
    (add_net "Net-(C16-Pad2)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C18-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C20-Pad2)")
    (add_net "Net-(C21-Pad2)")
    (add_net "Net-(C22-Pad1)")
    (add_net "Net-(C23-Pad1)")
    (add_net "Net-(C24-Pad1)")
    (add_net "Net-(C25-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(P10-Pad1)")
    (add_net "Net-(P17-Pad1)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R14-Pad2)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(R17-Pad1)")
    (add_net "Net-(R25-Pad2)")
    (add_net "Net-(R28-Pad1)")
    (add_net "Net-(R31-Pad1)")
    (add_net "Net-(R34-Pad1)")
    (add_net "Net-(R37-Pad1)")
  )
  (net_class GND ""
    (clearance 0.8)
    (trace_width 2)
    (via_dia 0.8)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net Earth)
    (add_net GND)
  )
  (net_class HT ""
    (clearance 1.8)
    (trace_width 0.8)
    (via_dia 0.8)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /HT_G2)
    (add_net /HT_U1A)
    (add_net /HT_U1B)
    (add_net /HT_U2A)
    (add_net /HT_U2B)
    (add_net /HT_U3A)
    (add_net /HT_U3B)
    (add_net /HT_U4A)
    (add_net /HT_U4B)
    (add_net /HT_U5B)
  )
  (module Mounting_Holes:MountingHole_3.5mm (layer F.Cu) (tedit 58EBF3F9)
    (at 292.9128 161.7472)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -0.4128 0.7528) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask)
      (clearance 2))
  )
  (module Mounting_Holes:MountingHole_3.5mm (layer F.Cu) (tedit 58EBF3D9)
    (at 247.6246 215.0618)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -0.1246 -0.0618) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask)
      (clearance 2))
  )
  (module Mounting_Holes:MountingHole_3.5mm (layer F.Cu) (tedit 58EBF338)
    (at 157.607 156.5148)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask)
      (clearance 2))
  )
  (module Mounting_Holes:MountingHole_3.5mm (layer F.Cu) (tedit 58EBF3C9)
    (at 83.7438 216.0524)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -1.2438 -0.0524) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask)
      (clearance 2))
  )
  (module Mounting_Holes:MountingHole_3.5mm (layer F.Cu) (tedit 58EBF363)
    (at 74.8792 105.156)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0.1208 -0.156) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask)
      (clearance 2))
  )
  (module Mounting_Holes:MountingHole_3.5mm (layer F.Cu) (tedit 58EBF368)
    (at 270.256 104.902)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -0.256 0.098) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask)
      (clearance 2))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 58EBCB4A)
    (at 92.4306 169.2148)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965_Pad (at 0 2.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 Earth))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 58EBCB4A)
    (at 337.6168 185.2422)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965_Pad (at 0 2.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 Earth))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 58EBCB4A)
    (at 337.4644 159.1564)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965_Pad (at 0 2.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 Earth))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 58EBCB4A)
    (at 234.7468 170.0784)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965_Pad (at 0 2.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 Earth))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 58EBCB4A)
    (at 122.8344 148.1328)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965_Pad (at 0 2.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 Earth))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 58EBCB4A)
    (at 92.9132 112.1918)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965_Pad (at 0 2.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 Earth))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 58EBCB4A)
    (at 239.141 111.7854)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965_Pad (at 0 2.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 Earth))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 58EBCB4A)
    (at 161.671 115.1382)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965_Pad (at 0 2.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 Earth))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 58EBCB4A)
    (at 137.6934 178.2826)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965_Pad (at 0 2.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 Earth))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 58EBCB4A)
    (at 175.387 216.2302)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965_Pad (at 0 2.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 Earth))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 58EBCB4A)
    (at 256.7432 208.4578)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_DIN965_Pad (at 0 2.9) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1 1) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 Earth))
  )
  (module A-wai_Turrets:TUBE_TRIODE (layer F.Cu) (tedit 58EBEFBA)
    (at 210 125)
    (descr Triode)
    (fp_text reference U5 (at -7.5 -17.5) (layer F.SilkS) hide)
    (fp_text value ECC83 (at -7.5 -15) (layer F.SilkS) hide)
    (pad 3 thru_hole circle (at -15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(R28-Pad1)") (clearance 0.5))
    (pad 8 thru_hole circle (at 15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(R10-Pad1)") (clearance 0.5))
    (pad "" np_thru_hole circle (at 0 0) (size 30 30) (drill 30) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 35 /HT_U5B))
    (pad 6 thru_hole circle (at 15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole circle (at 19 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C14-Pad2)"))
  )
  (module A-wai_Turrets:C_M150_105_100V (layer F.Cu) (tedit 57E564B1)
    (at 162.1282 122.3772 270)
    (descr "M150 1µF / 100V")
    (autoplace_cost180 10)
    (fp_text reference C17 (at 0 -1 270) (layer F.SilkS))
    (fp_text value 33n (at 0 1 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -12.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C17-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 12.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:TUBE_TRIODE (layer F.Cu) (tedit 58EBF102)
    (at 245 185)
    (descr Triode)
    (fp_text reference U2 (at -7.5 -17.5) (layer F.SilkS) hide)
    (fp_text value ECC83 (at -7.5 -15) (layer F.SilkS) hide)
    (pad 3 thru_hole circle (at -15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(C7-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at -19 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.5))
    (pad 8 thru_hole circle (at 15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(C3-Pad1)") (clearance 0.5))
    (pad "" np_thru_hole circle (at 0 0) (size 30 30) (drill 30) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 /HT_U2B))
    (pad 6 thru_hole circle (at 15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 /HT_U2A))
  )
  (module A-wai_Turrets:TUBE_TRIODE (layer F.Cu) (tedit 58EBF10B)
    (at 320 185)
    (descr Triode)
    (fp_text reference U1 (at -7.5 -17.5) (layer F.SilkS) hide)
    (fp_text value ECC83 (at -7.5 -15) (layer F.SilkS) hide)
    (pad 3 thru_hole circle (at -15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(R17-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at -19 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.5))
    (pad 8 thru_hole circle (at 15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(C13-Pad1)") (clearance 0.5))
    (pad "" np_thru_hole circle (at 0 0) (size 30 30) (drill 30) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 /HT_U1B))
    (pad 6 thru_hole circle (at 15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 /HT_U1A))
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 250.8758 124.3734 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R26 (at 0 2.286 270) (layer F.SilkS))
    (fp_text value 2.2M (at 0.1778 -0.0254 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C14-Pad1)"))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_225P_223_400V (layer F.Cu) (tedit 57D574FA)
    (at 223.647 212.5345 180)
    (descr "SBE 225P 22nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C8 (at 0.1016 1.1811 180) (layer F.SilkS))
    (fp_text value 22n (at 0 -0.7747 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 /HT_U2B))
    (pad 2 thru_hole circle (at 9.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C8-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_225P_473_400V (layer F.Cu) (tedit 57D57416)
    (at 295.3 209.423 180)
    (descr "SBE 225P 47nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C10 (at -0.0766 0.8382 180) (layer F.SilkS))
    (fp_text value 47n (at -0.2036 -1.3462 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 /HT_U1B))
    (pad 2 thru_hole circle (at 9.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C10-Pad2)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57E5A34D)
    (at 334.391 214.249)
    (descr Turret)
    (tags DEV)
    (fp_text reference P14 (at 0 -4.5) (layer Cmts.User))
    (fp_text value EARTH (at 0.127 4.064) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 31 Earth) (clearance 0.5))
  )
  (module A-wai_Turrets:C_225P_223_400V (layer F.Cu) (tedit 57D564C1)
    (at 199.0344 164.3888 270)
    (descr "SBE 225P 22nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C9 (at 0.0508 1.1176 270) (layer F.SilkS))
    (fp_text value 22n (at -0.2794 -1.1684 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 28 /HT_U3A) (clearance 0.5))
    (pad 2 thru_hole circle (at 9.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C11-Pad1)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_2W (layer F.Cu) (tedit 57D57142)
    (at 181.6872 148.1836)
    (descr "Resistance 2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R7 (at 0 -1) (layer F.SilkS))
    (fp_text value 10k/2W (at 0 1) (layer F.SilkS))
    (pad 1 thru_hole circle (at -8 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(C25-Pad1)"))
    (pad 2 thru_hole circle (at 8 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(C4-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 105.0902 131.1656 180)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R38 (at 0.112 2.413 180) (layer F.SilkS))
    (fp_text value 470k (at 0.127 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(C20-Pad2)"))
    (pad 2 thru_hole circle (at 7 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:CPA_22uF_450V (layer F.Cu) (tedit 57D5719A)
    (at 245.0465 184.3065 90)
    (descr "Capacitor F+T 22µF / 450V")
    (fp_text reference C1 (at -14.8295 10.4775 180) (layer F.SilkS))
    (fp_text value 22µ/450V (at -17.433 9.144 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 18 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at -19.2 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (clearance 0.5))
    (model walter/capacitors/cpa_13x31mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:CPA_33uF_500V (layer F.Cu) (tedit 57D57195)
    (at 175.006 184.2752 90)
    (descr "Capacitor F+T 22µF / 500V")
    (fp_text reference C2 (at -19.4328 11.176 360) (layer F.SilkS))
    (fp_text value 33µ/450V (at -21.9728 9.7028 360) (layer F.SilkS))
    (pad 1 thru_hole circle (at 22.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at -23.7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (clearance 0.5))
    (model walter/capacitors/cpa_13x31mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:CPA_47uF_450V (layer F.Cu) (tedit 57D57137)
    (at 104.2035 186.8805 90)
    (descr "Capacitor F+T 47µF / 450V")
    (fp_text reference C4 (at -19.6215 10.7315 180) (layer F.SilkS))
    (fp_text value 47µ/450V (at -22.1361 7.9121 360) (layer F.SilkS))
    (pad 1 thru_hole circle (at 22.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at -23.7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (clearance 0.5))
    (model walter/capacitors/cpa_13x31mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Passive:DIODE (layer F.Cu) (tedit 57BE0F22)
    (at 263.9695 112.3315 180)
    (descr "Diode 1N4007")
    (tags "DIODE DEV")
    (fp_text reference D1 (at 0 2.54 180) (layer F.SilkS))
    (fp_text value 1N4007 (at 0 -2.54 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 3.81 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(D1-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at -3.81 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(D1-Pad2)") (clearance 0.5))
    (model discret/diode.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Misc:relay-G5V2 (layer F.Cu) (tedit 57BDE8F3)
    (at 263.9695 125.5395 90)
    (descr RELAY)
    (tags RELAY)
    (attr virtual)
    (fp_text reference K1 (at -5.08 0 90) (layer F.SilkS))
    (fp_text value G5V2 (at 4.064 0.127 90) (layer F.SilkS))
    (pad 9 thru_hole oval (at -10.16 3.81 90) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
    (pad 11 thru_hole oval (at -5.08 3.81 90) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
    (pad 16 thru_hole oval (at 7.62 3.81 90) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(D1-Pad2)"))
    (pad 1 thru_hole oval (at 7.62 -3.81 90) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(D1-Pad1)"))
    (pad 6 thru_hole oval (at -5.08 -3.81 90) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C10-Pad2)"))
    (pad 8 thru_hole oval (at -10.16 -3.81 90) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 0 -3.81 90) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C14-Pad1)"))
    (pad 13 thru_hole oval (at 0 3.81 90) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57E5A2DB)
    (at 252.476 105.2068)
    (descr Turret)
    (tags DEV)
    (fp_text reference P1 (at 3.556 -3.175) (layer Cmts.User))
    (fp_text value RLY+ (at 0.254 -3.7846) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(D1-Pad1)") (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57E5A2DE)
    (at 262.4074 105.156)
    (descr Turret)
    (tags DEV)
    (fp_text reference P2 (at 0 -4.5) (layer Cmts.User))
    (fp_text value RLY- (at 0 -3.81) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(D1-Pad2)") (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57E5A328)
    (at 260.096 141.478)
    (descr Turret)
    (tags DEV)
    (fp_text reference P6 (at 0 -4.5) (layer Cmts.User))
    (fp_text value "FROM LD EQ" (at 8.1534 0.0508) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57E5A4D5)
    (at 152.6794 105.1814)
    (descr Turret)
    (tags DEV)
    (fp_text reference P11 (at 0 -4.5) (layer Cmts.User))
    (fp_text value Ug2 (at 0.0254 3.7338) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 /HT_G2))
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 213.599 163.1696)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R2 (at 0 -2.5) (layer F.SilkS))
    (fp_text value 10k (at -0.127 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(C1-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 138.8214 155.448)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R4 (at 0 -2.159) (layer F.SilkS))
    (fp_text value 10k (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(C2-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 260.2865 165.1)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R6 (at 0 -2.5) (layer F.SilkS))
    (fp_text value 220k (at 0.1397 0.0508) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 /HT_U2A))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 232.8164 124.968 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R8 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value 1M (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C14-Pad2)"))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(R10-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 239.8268 129.1394 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R11 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value 56k (at -0.127 -0.127 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(R10-Pad2)"))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(C15-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 221.8055 184.9905 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R13 (at -3.9139 -3.1115 540) (layer F.SilkS))
    (fp_text value 100k (at -0.4341 -0.1143 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 /HT_U2B))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 209.677 198.9605 90)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R14 (at -0.2009 -2.1082 90) (layer F.SilkS))
    (fp_text value 470k (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C8-Pad2)"))
    (pad 2 thru_hole circle (at 7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(R14-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 227.0125 204.597)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R15 (at 0 -2.5) (layer F.SilkS))
    (fp_text value 1M (at 0.254 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(R14-Pad2)"))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 197.6755 199.1995 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R16 (at 0.0635 2.1717 270) (layer F.SilkS))
    (fp_text value 39k (at 0 0.127 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(R16-Pad1)"))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 289.56 191.277 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R17 (at -0.015 2.286 270) (layer F.SilkS))
    (fp_text value 10k (at 0.0485 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(R17-Pad1)"))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 175.0164 157.0736)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R18 (at 0 -2.5) (layer F.SilkS))
    (fp_text value 100k (at -0.254 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 28 /HT_U3A))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 294.8305 184.9905 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R19 (at 0.2263 -2.2733 270) (layer F.SilkS))
    (fp_text value 100k (at 0.0485 -0.0889 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 /HT_U1B))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 304.8635 203.581)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R21 (at 0 -2.5) (layer F.SilkS))
    (fp_text value 2.2M (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C10-Pad2)"))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 150.622 185.0748 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R24 (at 3.0122 -2.2352 270) (layer F.SilkS))
    (fp_text value 220k (at 0.015 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 29 /HT_U3B))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 136.2964 200.2028 90)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R25 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value 1M (at -0.0762 0.0254 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C16-Pad2)"))
    (pad 2 thru_hole circle (at 7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(R25-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 156.972 203.2)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R27 (at -0.3048 -2.3876) (layer F.SilkS))
    (fp_text value 100k (at -0.097 -0.127) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(R25-Pad2)"))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 179.8066 117.9068 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R28 (at 2.1082 0.0254 270) (layer F.SilkS))
    (fp_text value 1k (at -2.9464 -0.1016 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(R28-Pad1)"))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(P10-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 175.5394 125.0696 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R29 (at 0.0254 2.0066 270) (layer F.SilkS))
    (fp_text value 470R (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(P10-Pad1)"))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 184.6326 125.0188 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R30 (at -0.0762 -2.413 270) (layer F.SilkS))
    (fp_text value 100k (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 35 /HT_U5B))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 120.5484 203.0476 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R31 (at 0.0254 2.3622 270) (layer F.SilkS))
    (fp_text value 2.2k (at -0.1524 0.0254 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(R31-Pad1)"))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 119.5832 164.3126)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R32 (at 0.0762 2.3114) (layer F.SilkS))
    (fp_text value 220k (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 /HT_U4A))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 132.5626 178.4962 90)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R34 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value 1M (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(R34-Pad1)"))
    (pad 2 thru_hole circle (at 7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(C18-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 76.7842 194.2442 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R37 (at 0.0912 2.2098 270) (layer F.SilkS))
    (fp_text value 2.2k (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(R37-Pad1)"))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:TUBE_PENTODE (layer F.Cu) (tedit 57E5A2D0)
    (at 140 125)
    (descr Pentode)
    (fp_text reference U6 (at -10 -17.5) (layer Cmts.User))
    (fp_text value 6V6 (at -10 -15) (layer Cmts.User))
    (pad 3 thru_hole circle (at 0 -19) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(C22-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at -13.5 13.5) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(C20-Pad2)") (clearance 0.5))
    (pad 9 thru_hole circle (at 13.5 13.5) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 /HT_G2))
    (pad "" np_thru_hole circle (at 0 0) (size 30 30) (drill 30) (layers *.Cu *.Mask F.SilkS))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57E5A314)
    (at 280.0985 192.5955)
    (descr Turret)
    (tags DEV)
    (fp_text reference P15 (at 0 -4.5) (layer Cmts.User))
    (fp_text value "LD GND" (at 0 3.683) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (clearance 0.5))
  )
  (module Freetronics:SJ_OPEN (layer F.Cu) (tedit 54779663)
    (at 334.391 209.55 270)
    (descr "<b>Solder jumper</b>")
    (fp_text reference JP1 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value JUMPER (at 0 1.6 270) (layer Eco1.User) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 1.1684 1.6002) (layers F.Cu F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 1.1684 1.6002) (layers F.Cu F.Mask)
      (net 31 Earth))
  )
  (module A-wai_Turrets:C_225P_472_400V (layer F.Cu) (tedit 57E5649E)
    (at 280.035 174.8155 270)
    (descr "SBE 225P 4.7nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C6 (at 4.826 1.3335 270) (layer F.SilkS))
    (fp_text value 2.2n (at -3.81 1.2065 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C5-Pad2)") (clearance 0.5))
    (pad 2 thru_hole circle (at 9.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(C6-Pad2)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_M150_105_100V (layer F.Cu) (tedit 57E564B1)
    (at 215.4555 185.112 270)
    (descr "M150 1µF / 100V")
    (autoplace_cost180 10)
    (fp_text reference C7 (at 3.3655 0.889 270) (layer F.SilkS))
    (fp_text value 1µ (at -2.7305 1.0795 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -12.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(C7-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 12.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_225P_472_400V (layer F.Cu) (tedit 57E5649E)
    (at 203.581 190.4365 270)
    (descr "SBE 225P 4.7nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C11 (at 4.0005 1.0795 270) (layer F.SilkS))
    (fp_text value 1n (at -2.9845 1.397 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C11-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 9.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_M150_105_100V (layer F.Cu) (tedit 57E564B1)
    (at 144.2212 185.0136 270)
    (descr "M150 1µF / 100V")
    (autoplace_cost180 10)
    (fp_text reference C12 (at 3.2258 0.9652 270) (layer F.SilkS))
    (fp_text value 1µ (at -2.7178 1.1684 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -12.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(C12-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 12.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:CPA_22uF_63V (layer F.Cu) (tedit 58DAB62D)
    (at 343.916 203.249 90)
    (descr "Capacitor axial 22µF / 63V")
    (fp_text reference C13 (at -4.015 -1.9685 90) (layer F.SilkS))
    (fp_text value 22µ (at 1.954 -2.032 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 9.8 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(C13-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at -11 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (clearance 0.5))
    (model walter/capacitors/cpa_13x31mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:CPA_22uF_63V (layer F.Cu) (tedit 558FF971)
    (at 259.2368 147.9804)
    (descr "Capacitor axial 22µF / 63V")
    (fp_text reference C15 (at -0.0298 -1.778) (layer F.SilkS))
    (fp_text value 10µ/160V (at -0.106 2.159) (layer F.SilkS))
    (pad 1 thru_hole circle (at 9.8 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(C15-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at -11 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(C15-Pad2)") (clearance 0.5))
    (model walter/capacitors/cpa_13x31mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_225P_223_400V (layer F.Cu) (tedit 57E56479)
    (at 153.0096 211.2264 180)
    (descr "SBE 225P 22nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C16 (at 0.2286 1.0414 180) (layer F.SilkS))
    (fp_text value 22n (at -0.1524 -1.143 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 29 /HT_U3B) (clearance 0.5))
    (pad 2 thru_hole circle (at 9.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C16-Pad2)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_225P_223_400V (layer F.Cu) (tedit 57E56479)
    (at 129.2098 159.8168)
    (descr "SBE 225P 22nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C18 (at 0 -1) (layer F.SilkS))
    (fp_text value 22n (at 0 1) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 /HT_U4A) (clearance 0.5))
    (pad 2 thru_hole circle (at 9.5 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(C18-Pad2)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_225P_473_400V (layer F.Cu) (tedit 57E564A9)
    (at 150.52 144.0688 180)
    (descr "SBE 225P 47nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C20 (at 0.0758 1.143 180) (layer F.SilkS))
    (fp_text value 47n (at 0.025 -1.2954 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 35 /HT_U5B) (clearance 0.5))
    (pad 2 thru_hole circle (at 9.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(C20-Pad2)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_225P_223_400V (layer F.Cu) (tedit 57E56479)
    (at 84.099 212.852 180)
    (descr "SBE 225P 22nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C21 (at -3.8358 1.5748 180) (layer F.SilkS))
    (fp_text value 22n (at -4.1406 -0.762 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 /HT_U4B) (clearance 0.5))
    (pad 2 thru_hole circle (at 9.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(C21-Pad2)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_225P_103_400V (layer F.Cu) (tedit 57E56458)
    (at 82.825776 152.748532 180)
    (descr "SBE 225P 10nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C23 (at 0.097976 1.186732 180) (layer F.SilkS))
    (fp_text value 10n (at 0.097976 -0.921468 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(C23-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 9.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:CPA_22uF_450V (layer F.Cu) (tedit 558F0D82)
    (at 320.167 184.381 90)
    (descr "Capacitor F+T 22µF / 450V")
    (fp_text reference C24 (at -14.628 10.668 180) (layer F.SilkS))
    (fp_text value 22µ/450V (at -17.168 8.1915 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 18 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(C24-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at -19.2 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (clearance 0.5))
    (model walter/capacitors/cpa_13x31mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:CPA_47uF_450V (layer F.Cu) (tedit 558F0E57)
    (at 210.2358 125.9822 90)
    (descr "Capacitor F+T 47µF / 450V")
    (fp_text reference C25 (at 0 -11 90) (layer F.SilkS))
    (fp_text value 47µ/450V (at 0 11 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 22.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(C25-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at -23.7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (clearance 0.5))
    (model walter/capacitors/cpa_13x31mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 58EBF171)
    (at 343.916 174.117)
    (descr Turret)
    (tags DEV)
    (fp_text reference P4 (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value "CLN EQ" (at -0.1524 3.937) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 /HT_U1A) (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 58BF2FEE)
    (at 343.916 182.8165)
    (descr Turret)
    (tags DEV)
    (fp_text reference P16 (at 4.3815 0.0635) (layer F.SilkS) hide)
    (fp_text value "CLN EQ GND" (at 0.1905 3.7465) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 58EBEF61)
    (at 76.3016 135.4074)
    (descr Turret)
    (tags DEV)
    (fp_text reference P17 (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value "LD EQ" (at 0.0762 -4.4196) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(P17-Pad1)") (clearance 0.5))
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 336.931 165.735)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R3 (at 0.0635 -2.413) (layer F.SilkS))
    (fp_text value 100k (at 0.127 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 /HT_U1A))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 227.965 143.2306)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R10 (at 0 -2.5) (layer F.SilkS))
    (fp_text value 1.5k (at 0.1016 0.0254) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(R10-Pad1)"))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(R10-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 239.8268 143.1394 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R22 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value 47k (at -0.0612 0.0254 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(C15-Pad1)"))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 81.2546 201.168 90)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R35 (at 0.0508 2.3876 90) (layer F.SilkS))
    (fp_text value 1M (at -0.0254 0.0508 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(C21-Pad2)"))
    (pad 2 thru_hole circle (at 7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(R34-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 127.9906 199.2526 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R36 (at -0.015 2.3368 270) (layer F.SilkS))
    (fp_text value 1M (at 0.0612 -0.0508 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(R34-Pad1)"))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 78.5876 173.0756 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R39 (at -0.0508 2.2098 270) (layer F.SilkS))
    (fp_text value 100k (at -0.127 -0.0508 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 /HT_U4B))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 105.827776 147.109732 180)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R41 (at -0.039424 2.202732 180) (layer F.SilkS))
    (fp_text value 82k (at 0.036776 -0.083268 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(P17-Pad1)"))
    (pad 2 thru_hole circle (at 7 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(C21-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 83.384576 144.976132 180)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R42 (at -0.054424 2.431332 180) (layer F.SilkS))
    (fp_text value 47k (at 0.072576 0.018332 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(P17-Pad1)"))
    (pad 2 thru_hole circle (at 7 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 99.223776 152.799332 180)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R43 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value 33k (at -0.039424 -0.083268 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(P17-Pad1)"))
    (pad 2 thru_hole circle (at 7 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(C23-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 319.9765 154.94)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R44 (at 0 -2.5) (layer F.SilkS))
    (fp_text value 10k (at -0.0381 0.0508) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(C4-Pad1)"))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(C24-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_2W (layer F.Cu) (tedit 57BE1221)
    (at 180.3664 104.1908)
    (descr "Resistance 2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R45 (at 0 -1) (layer F.SilkS))
    (fp_text value 10k/2W (at 0 1) (layer F.SilkS))
    (pad 1 thru_hole circle (at -8 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 45 /HT) (clearance 0.5))
    (pad 2 thru_hole circle (at 8 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(C25-Pad1)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:TUBE_TRIODE (layer F.Cu) (tedit 58EBF438)
    (at 175 185)
    (descr Triode)
    (fp_text reference U3 (at -7.5 -17.5) (layer F.SilkS) hide)
    (fp_text value ECC83 (at -7.5 -15) (layer F.SilkS) hide)
    (pad 3 thru_hole circle (at -15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(C12-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at -19 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C11-Pad1)") (clearance 0.5))
    (pad 8 thru_hole circle (at 15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(R16-Pad1)") (clearance 0.5))
    (pad "" np_thru_hole circle (at 0 0) (size 30 30) (drill 30) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 29 /HT_U3B))
    (pad 6 thru_hole circle (at 15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 28 /HT_U3A))
    (pad 7 thru_hole circle (at 19 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(R14-Pad2)"))
  )
  (module A-wai_Turrets:TUBE_TRIODE (layer F.Cu) (tedit 58EBEF1D)
    (at 105 185)
    (descr Triode)
    (fp_text reference U4 (at -7.5 -17.5) (layer F.SilkS) hide)
    (fp_text value ECC83 (at -7.5 -15) (layer F.SilkS) hide)
    (pad 3 thru_hole circle (at -15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(R37-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at -19 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(R34-Pad1)") (clearance 0.5))
    (pad 8 thru_hole circle (at 15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(R31-Pad1)") (clearance 0.5))
    (pad "" np_thru_hole circle (at 0 0) (size 30 30) (drill 30) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 /HT_U4B))
    (pad 6 thru_hole circle (at 15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 /HT_U4A))
    (pad 7 thru_hole circle (at 19 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(R25-Pad2)"))
  )
  (module A-wai_Turrets:C_M150_105_100V (layer F.Cu) (tedit 57E564B1)
    (at 267.335 196.5865 270)
    (descr "M150 1µF / 100V")
    (autoplace_cost180 10)
    (fp_text reference C3 (at 4.4545 2.2225 270) (layer F.SilkS))
    (fp_text value 1µ (at -4.0545 2.4765 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -12.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(C3-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 12.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND) (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_225P_223_400V (layer F.Cu) (tedit 57E56479)
    (at 273.558 169.3795 90)
    (descr "SBE 225P 22nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C5 (at 0 -1 90) (layer F.SilkS))
    (fp_text value 22n (at 0 1 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 /HT_U2A) (clearance 0.5))
    (pad 2 thru_hole circle (at 9.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C5-Pad2)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_225P_103_400V (layer F.Cu) (tedit 57E56458)
    (at 234.7718 104.1654 180)
    (descr "SBE 225P 10nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C14 (at -0.0766 1.1684 180) (layer F.SilkS))
    (fp_text value 10n (at -0.1782 -1.1176 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C14-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 9.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C14-Pad2)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.5mm (layer F.Cu) (tedit 58EBF385)
    (at 345.1352 151.8666)
    (descr "Mounting Hole 3.5mm, no annular")
    (tags "mounting hole 3.5mm no annular")
    (fp_text reference REF** (at 0 -4.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.5mm (at 0 4.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at -0.1352 0.6334) (size 3.5 3.5) (drill 3.5) (layers *.Cu *.Mask)
      (clearance 2))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57BE120D)
    (at 168.9608 125.095)
    (descr Turret)
    (tags DEV)
    (fp_text reference P10 (at 0 -4.5) (layer F.SilkS))
    (fp_text value DEPTH (at 0 5) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(P10-Pad1)") (clearance 0.5))
  )
  (gr_text "LD GAIN" (at 226.1108 188.6712) (layer F.SilkS))
  (gr_text DEPTH (at 169.6466 108.7882) (layer F.SilkS))
  (gr_text "R23  1.8k" (at 145.669 184.8612 90) (layer F.SilkS))
  (gr_text "R20   330k" (at 205.105 190.4365 90) (layer F.SilkS))
  (gr_text "R12   1.8k" (at 216.789 185.1025 90) (layer F.SilkS))
  (gr_text "R1  1.5k" (at 345.948 204.4065 90) (layer F.SilkS))
  (gr_text "R9   470k" (at 281.4955 174.752 90) (layer F.SilkS))
  (gr_text "R5    1.8k" (at 269.9385 196.7865 90) (layer F.SilkS))
  (gr_text "Evil Eddie\nA-wai Amplification" (at 104.4448 113.9952) (layer F.SilkS))
  (gr_text PRSNC (at 163.4744 103.3272) (layer F.SilkS))
  (gr_text "CLN VOL" (at 300.99 188.976) (layer F.SilkS))
  (gr_text "TO MSTR" (at 275.7424 148.6154) (layer F.SilkS))
  (gr_text C+ (at 168.1226 101.981) (layer F.SilkS))
  (gr_text "TO LD GAIN" (at 280.3525 188.341) (layer F.SilkS))
  (gr_line (start 347 220) (end 350 217) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 70 217) (end 73 220) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 70 103) (end 73 100) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 347 147) (end 350 150) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 272 100) (end 275 103) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 275 130) (end 285 140) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 302 147) (end 347 147) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 295 140) (end 302 147) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 285 140) (end 295 140) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 275 103) (end 275 130) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 70 103) (end 70 217) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 272 100) (end 73 100) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 350 217) (end 350 150) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73 220) (end 347 220) (layer Edge.Cuts) (width 0.1))
  (zone (net 31) (net_name Earth) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.8))
    (min_thickness 0.5)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 354.253676 96.647) (xy 352.729676 221.996) (xy 63.804676 225.933) (xy 61.772676 96.647)
      )
    )
  )
  (zone (net 31) (net_name Earth) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.8))
    (min_thickness 0.5)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 58.674 90.678) (xy 361.569 94.615) (xy 357.124 225.298) (xy 53.848 231.902) (xy 56.515 91.313)
      )
    )
  )
)
