(kicad_pcb (version 4) (host pcbnew 4.0.4+dfsg1-stable)
  (general
    (links 102)
    (no_connects 7)
    (area 69.949999 99.949999 350.050001 220.050001)
    (thickness 1.6)
    (drawings 29)
    (tracks 281)
    (zones 0)
    (modules 71)
    (nets 46)
  )
  (page A3)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.8)
    (trace_clearance 0.8)
    (zone_clearance 0.8)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.8)
    (via_drill 0.6)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.2 3.2)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerber/))
  )
  (net 0 "")
  (net 1 F+)
  (net 2 GND)
  (net 3 E+)
  (net 4 D+)
  (net 5 /HT_U1A)
  (net 6 "Net-(C5-Pad2)")
  (net 7 /HT_U2A)
  (net 8 "Net-(C8-Pad2)")
  (net 9 /HT_U2B)
  (net 10 "Net-(C11-Pad1)")
  (net 11 /HT_U1B)
  (net 12 "Net-(C10-Pad2)")
  (net 13 "Net-(C14-Pad1)")
  (net 14 "Net-(C14-Pad2)")
  (net 15 /HT_U4B)
  (net 16 "Net-(C16-Pad2)")
  (net 17 "Net-(C17-Pad1)")
  (net 18 /HT_U4A)
  (net 19 "Net-(C18-Pad2)")
  (net 20 "Net-(C19-Pad1)")
  (net 21 "Net-(C19-Pad2)")
  (net 22 "Net-(C20-Pad1)")
  (net 23 "Net-(C20-Pad2)")
  (net 24 "Net-(D1-Pad1)")
  (net 25 "Net-(D1-Pad2)")
  (net 26 "Net-(C6-Pad1)")
  (net 27 "Net-(K1-Pad11)")
  (net 28 "Net-(K1-Pad8)")
  (net 29 "Net-(K1-Pad4)")
  (net 30 C+)
  (net 31 "Net-(C6-Pad2)")
  (net 32 "Net-(P7-Pad1)")
  (net 33 /HT_G2)
  (net 34 "Net-(P12-Pad1)")
  (net 35 "Net-(C3-Pad1)")
  (net 36 "Net-(C7-Pad1)")
  (net 37 "Net-(R14-Pad2)")
  (net 38 "Net-(R16-Pad1)")
  (net 39 "Net-(R17-Pad1)")
  (net 40 "Net-(C12-Pad1)")
  (net 41 /HT_U3A)
  (net 42 /HT_U3B)
  (net 43 "Net-(R29-Pad1)")
  (net 44 "Net-(R31-Pad1)")
  (net 45 Earth)
  (net_class Default "This is the default net class."
    (clearance 0.8)
    (trace_width 0.8)
    (via_dia 0.8)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net Earth)
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C14-Pad2)")
    (add_net "Net-(C16-Pad2)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C18-Pad2)")
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C19-Pad2)")
    (add_net "Net-(C20-Pad1)")
    (add_net "Net-(C20-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(K1-Pad11)")
    (add_net "Net-(K1-Pad4)")
    (add_net "Net-(K1-Pad8)")
    (add_net "Net-(P12-Pad1)")
    (add_net "Net-(P7-Pad1)")
    (add_net "Net-(R14-Pad2)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(R17-Pad1)")
    (add_net "Net-(R29-Pad1)")
    (add_net "Net-(R31-Pad1)")
  )
  (net_class GND ""
    (clearance 0.8)
    (trace_width 2)
    (via_dia 0.8)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (net_class HT ""
    (clearance 1.8)
    (trace_width 0.8)
    (via_dia 0.8)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /HT_G2)
    (add_net /HT_U1A)
    (add_net /HT_U1B)
    (add_net /HT_U2A)
    (add_net /HT_U2B)
    (add_net /HT_U3A)
    (add_net /HT_U3B)
    (add_net /HT_U4A)
    (add_net /HT_U4B)
    (add_net C+)
    (add_net D+)
    (add_net E+)
    (add_net F+)
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 146.685 188.849 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R26 (at 0 2.286 270) (layer F.SilkS))
    (fp_text value 2.2M (at -0.127 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(K1-Pad4)"))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 57E5A6AC)
    (at 210 165)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference REF (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value ø3.2 (at 0 2.413) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu F.SilkS)
      (clearance 2))
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 57E5A6AC)
    (at 345 152)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference REF (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value ø3.2 (at 0 2.413) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu F.SilkS)
      (clearance 2))
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 57E5A6AC)
    (at 270 105)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference REF (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value ø3.2 (at 0 2.413) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu F.SilkS)
      (clearance 2))
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 57E5A6AC)
    (at 75 105)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference REF (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value ø3.2 (at 0 2.413) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu F.SilkS)
      (clearance 2))
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 57E5A6AC)
    (at 75 215)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference REF (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value ø3.2 (at 0 2.413) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu F.SilkS)
      (clearance 2))
  )
  (module A-wai_Turrets:C_225P_472_400V (layer F.Cu) (tedit 57E5642E)
    (at 259.969 132.74 90)
    (descr "SBE 225P 4.7nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference R9 (at 0 -1 90) (layer F.SilkS))
    (fp_text value 1M (at 0 1 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(C6-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 9.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(C6-Pad2)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_M150_105_100V (layer F.Cu) (tedit 57E56423)
    (at 343.916 201.749 270)
    (descr "M150 1µF / 100V")
    (autoplace_cost180 10)
    (fp_text reference R5 (at 2.34 1.016 270) (layer F.SilkS))
    (fp_text value 1.8k (at -2.74 1.016 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -12.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(C3-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 12.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_M150_105_100V (layer F.Cu) (tedit 57E56413)
    (at 275.336 212.598 180)
    (descr "M150 1µF / 100V")
    (autoplace_cost180 10)
    (fp_text reference R12 (at 2.667 1.143 180) (layer F.SilkS))
    (fp_text value 1.8k (at -2.794 1.143 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -12.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(C7-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 12.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_M150_105_100V (layer F.Cu) (tedit 57E56406)
    (at 175.714 216.662)
    (descr "M150 1µF / 100V")
    (autoplace_cost180 10)
    (fp_text reference R23 (at -2.359 -1.778) (layer F.SilkS))
    (fp_text value 1.8k (at 3.102 -1.778) (layer F.SilkS))
    (pad 1 thru_hole circle (at -12.5 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(C12-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 12.5 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_225P_472_400V (layer F.Cu) (tedit 57E5639E)
    (at 202.184 199.644 270)
    (descr "SBE 225P 4.7nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference R20 (at 3.175 3.937 270) (layer F.SilkS))
    (fp_text value 330k (at -3.048 4.064 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C11-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 9.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_225P_223_400V (layer F.Cu) (tedit 57D574FA)
    (at 250.063 160.02 180)
    (descr "SBE 225P 22nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C8 (at 0 -1 180) (layer F.SilkS))
    (fp_text value 22n (at 0 1 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 /HT_U2A))
    (pad 2 thru_hole circle (at 9.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C8-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_225P_473_400V (layer F.Cu) (tedit 57D574D7)
    (at 109.093 159.004 180)
    (descr "SBE 225P 47nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C18 (at 0 -1 180) (layer F.SilkS))
    (fp_text value 47n (at 0 1 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 /HT_U4A))
    (pad 2 thru_hole circle (at 9.5 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(C18-Pad2)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_225P_473_400V (layer F.Cu) (tedit 57D57416)
    (at 281.432 182.626 90)
    (descr "SBE 225P 47nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C10 (at 0 -1 90) (layer F.SilkS))
    (fp_text value 47n (at 0 1 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 /HT_U1B))
    (pad 2 thru_hole circle (at 9.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C10-Pad2)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_225P_104_400V (layer F.Cu) (tedit 57D57405)
    (at 170.18 122.428 90)
    (descr "SBE 225P 100nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C20 (at 0 -1 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(C20-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 9.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(C20-Pad2)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_225P_104_400V (layer F.Cu) (tedit 57D573FD)
    (at 96.647 129.032 270)
    (descr "SBE 225P 100nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C19 (at 0 -1 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(C19-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 9.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(C19-Pad2)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_225P_473_400V (layer F.Cu) (tedit 57D573E0)
    (at 75.692 185.293 270)
    (descr "SBE 225P 47nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C16 (at 0 -1 270) (layer F.SilkS))
    (fp_text value 47n (at 0 1 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 /HT_U4B))
    (pad 2 thru_hole circle (at 9.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(C16-Pad2)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_225P_104_400V (layer F.Cu) (tedit 57D573D0)
    (at 105.816 213.36)
    (descr "SBE 225P 100nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C17 (at 0 -1) (layer F.SilkS))
    (fp_text value 100n (at 0 1) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(C17-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 9.5 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_225P_103_400V (layer F.Cu) (tedit 57D572D9)
    (at 134.366 172.339 270)
    (descr "SBE 225P 10nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C14 (at 0 1.016 270) (layer F.SilkS))
    (fp_text value 10n (at 0 -1.016 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C14-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at 9.5 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C14-Pad2)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57E5A34D)
    (at 334.391 214.249)
    (descr Turret)
    (tags DEV)
    (fp_text reference P14 (at 0 -4.5) (layer Cmts.User))
    (fp_text value EARTH (at 0.127 4.064) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 3.2) (layers *.Cu *.Mask F.SilkS)
      (net 45 Earth) (clearance 0.5))
  )
  (module A-wai_Turrets:C_225P_104_400V (layer F.Cu) (tedit 57D571BC)
    (at 344.17 170.307 90)
    (descr "SBE 225P 100nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C5 (at 0 -1 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 /HT_U1A))
    (pad 2 thru_hole circle (at 9.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C5-Pad2)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:C_225P_223_400V (layer F.Cu) (tedit 57D564C1)
    (at 205.359 189.611 90)
    (descr "SBE 225P 22nF / 400V")
    (autoplace_cost180 10)
    (fp_text reference C9 (at 7.874 -4.318 90) (layer F.SilkS))
    (fp_text value 22n (at 7.62 4.445 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -9.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 /HT_U2B) (clearance 0.5))
    (pad 2 thru_hole circle (at 9.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C11-Pad1)") (clearance 0.5))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_2W (layer F.Cu) (tedit 57D57142)
    (at 159.766 159.385)
    (descr "Resistance 2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R7 (at 0 -1) (layer F.SilkS))
    (fp_text value 10k/2W (at 0 1) (layer F.SilkS))
    (pad 1 thru_hole circle (at -8 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 30 C+))
    (pad 2 thru_hole circle (at 8 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 D+))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:TUBE_TRIODE (layer F.Cu) (tedit 57E5A270)
    (at 105 185)
    (descr Triode)
    (fp_text reference U4 (at -1.114 -18.249) (layer Cmts.User))
    (fp_text value ECC83 (at -1.114 -16.344) (layer Cmts.User))
    (pad 2 thru_hole circle (at -19 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(C17-Pad1)") (clearance 0.5))
    (pad 8 thru_hole circle (at 15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(R31-Pad1)") (clearance 0.5))
    (pad "" np_thru_hole circle (at 0 0) (size 30 30) (drill 30) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 /HT_U4B))
    (pad 6 thru_hole circle (at 15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 /HT_U4A))
    (pad 7 thru_hole circle (at 19 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C14-Pad2)"))
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 170.18 138.43 180)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R38 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value 100k (at 0.127 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(C20-Pad1)"))
    (pad 2 thru_hole circle (at 7 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(P12-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:TUBE_TRIODE (layer F.Cu) (tedit 57E5A279)
    (at 175 185)
    (descr Triode)
    (fp_text reference U3 (at -7.5 -17.5) (layer Cmts.User))
    (fp_text value ECC83 (at -7.5 -15) (layer Cmts.User))
    (pad 3 thru_hole circle (at -15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 42 /HT_U3B))
    (pad 8 thru_hole circle (at 15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(C12-Pad1)") (clearance 0.5))
    (pad "" np_thru_hole circle (at 0 0) (size 30 30) (drill 30) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 D+))
    (pad 6 thru_hole circle (at 15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 41 /HT_U3A))
    (pad 7 thru_hole circle (at 19 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C11-Pad1)"))
  )
  (module A-wai_Turrets:TUBE_TRIODE (layer F.Cu) (tedit 57E5A35A)
    (at 320 185)
    (descr Triode)
    (fp_text reference U1 (at -7.5 -17.5) (layer Cmts.User))
    (fp_text value ECC83 (at -7.5 -15) (layer Cmts.User))
    (pad 3 thru_hole circle (at -15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(R17-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at -19 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (clearance 0.5))
    (pad 8 thru_hole circle (at 15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(C3-Pad1)") (clearance 0.5))
    (pad "" np_thru_hole circle (at 0 0) (size 30 30) (drill 30) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 /HT_U1B))
    (pad 6 thru_hole circle (at 15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 /HT_U1A))
  )
  (module A-wai_Turrets:CPA_22uF_450V (layer F.Cu) (tedit 57D5719A)
    (at 320.04 184.381 90)
    (descr "Capacitor F+T 22µF / 450V")
    (fp_text reference C1 (at -15.263 -10.414 180) (layer F.SilkS))
    (fp_text value 22µ/450V (at -17.93 -8.89 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 18 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 F+))
    (pad 2 thru_hole circle (at -19.2 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (model walter/capacitors/cpa_13x31mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:CPA_33uF_500V (layer F.Cu) (tedit 57D57195)
    (at 250.063 189.025 90)
    (descr "Capacitor F+T 22µF / 500V")
    (fp_text reference C2 (at -14.683 -13.335 90) (layer F.SilkS))
    (fp_text value 33µ/450V (at -14.683 -10.668 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 22.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 E+))
    (pad 2 thru_hole circle (at -23.7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (model walter/capacitors/cpa_13x31mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:CPA_47uF_450V (layer F.Cu) (tedit 57D57137)
    (at 175.7426 186.965 90)
    (descr "Capacitor F+T 47µF / 450V")
    (fp_text reference C4 (at -15.6 -13.4366 90) (layer F.SilkS))
    (fp_text value 47µ/450V (at -15.6 -11.1506 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at 22.5 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 D+))
    (pad 2 thru_hole circle (at -23.7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (model walter/capacitors/cpa_13x31mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Passive:DIODE (layer F.Cu) (tedit 57BE0F22)
    (at 247.396 118.872 180)
    (descr "Diode 1N4007")
    (tags "DIODE DEV")
    (fp_text reference D1 (at 0 2.54 180) (layer F.SilkS))
    (fp_text value 1N4007 (at 0 -2.54 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 3.81 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(D1-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at -3.81 0 180) (size 2 2) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(D1-Pad2)") (clearance 0.5))
    (model discret/diode.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Misc:relay-G5V2 (layer F.Cu) (tedit 57BDE8F3)
    (at 247.396 132.08 90)
    (descr RELAY)
    (tags RELAY)
    (attr virtual)
    (fp_text reference K1 (at -5.08 0 90) (layer F.SilkS))
    (fp_text value G5V2 (at 4.064 0.127 90) (layer F.SilkS))
    (pad 9 thru_hole oval (at -10.16 3.81 90) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(C6-Pad1)"))
    (pad 11 thru_hole oval (at -5.08 3.81 90) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(K1-Pad11)"))
    (pad 16 thru_hole oval (at 7.62 3.81 90) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(D1-Pad2)"))
    (pad 1 thru_hole oval (at 7.62 -3.81 90) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(D1-Pad1)"))
    (pad 6 thru_hole oval (at -5.08 -3.81 90) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C10-Pad2)"))
    (pad 8 thru_hole oval (at -10.16 -3.81 90) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(K1-Pad8)"))
    (pad 4 thru_hole oval (at 0 -3.81 90) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(K1-Pad4)"))
    (pad 13 thru_hole oval (at 0 3.81 90) (size 2.5 4) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C5-Pad2)"))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57E5A2DB)
    (at 231.394 118.872)
    (descr Turret)
    (tags DEV)
    (fp_text reference P1 (at 3.556 -3.175) (layer Cmts.User))
    (fp_text value RLY+ (at 0 3.937) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(D1-Pad1)") (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57E5A2DE)
    (at 231.394 108.966)
    (descr Turret)
    (tags DEV)
    (fp_text reference P2 (at 0 -4.5) (layer Cmts.User))
    (fp_text value RLY- (at 0 -3.81) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(D1-Pad2)") (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57E5A2AA)
    (at 75.819 161.163)
    (descr Turret)
    (tags DEV)
    (fp_text reference P3 (at 0 -4.5) (layer Cmts.User))
    (fp_text value HT (at 0 4.064) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 30 C+))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57E5A328)
    (at 234.569 142.24)
    (descr Turret)
    (tags DEV)
    (fp_text reference P6 (at 0 -4.5) (layer Cmts.User))
    (fp_text value "FROM LD EQ" (at 0 4.572) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(K1-Pad8)") (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57E5A0E1)
    (at 95.631 168.275)
    (descr Turret)
    (tags DEV)
    (fp_text reference P9 (at 0 -4.5) (layer Cmts.User))
    (fp_text value "TO PA+" (at 0 -3.937) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(C18-Pad2)") (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57E5A290)
    (at 96.647 109.855)
    (descr Turret)
    (tags DEV)
    (fp_text reference P10 (at 0 -4.5) (layer Cmts.User))
    (fp_text value "FROM PRE+" (at 0 -4.064) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(C19-Pad1)") (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57E5A4D5)
    (at 75.819 146.05)
    (descr Turret)
    (tags DEV)
    (fp_text reference P11 (at 0 -4.5) (layer Cmts.User))
    (fp_text value Ug2 (at 0 3.937) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 33 /HT_G2))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57E5A4CF)
    (at 75.819 117.475)
    (descr Turret)
    (tags DEV)
    (fp_text reference P12 (at 0 -4.5) (layer Cmts.User))
    (fp_text value Ubias (at 0 4.191) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(P12-Pad1)") (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57E5A2BA)
    (at 160.401 112.903)
    (descr Turret)
    (tags DEV)
    (fp_text reference P13 (at 0 -4.5) (layer Cmts.User))
    (fp_text value "FROM PRE-" (at 0 -3.81) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(C20-Pad2)") (clearance 0.5))
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 304.8 158.369)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R2 (at 0 -2.5) (layer F.SilkS))
    (fp_text value 10k (at -0.127 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 E+))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 F+))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 216.154 154.432)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R4 (at 0 -2.159) (layer F.SilkS))
    (fp_text value 10k (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 D+))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 E+))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 328.407 156.972)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R6 (at 0 -2.5) (layer F.SilkS))
    (fp_text value 220k (at -0.112 0.254) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 F+))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 /HT_U1A))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 317.866 214.249 180)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R8 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value 2.2M (at 0 0 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C5-Pad2)"))
    (pad 2 thru_hole circle (at 7 0 180) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 291.211 158.242 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R11 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value 2.2M (at -0.127 -0.127 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(K1-Pad11)"))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 273.177 161.544 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R13 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value 100k (at -0.127 -0.254 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 E+))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 /HT_U2A))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 224.663 171.054 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R14 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value 470k (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C8-Pad2)"))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(R14-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 224.663 185.039 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R15 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value 1M (at 0.254 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(R14-Pad2)"))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 211.709 199.009 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R16 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value 39k (at 0 0.127 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(R16-Pad1)"))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 287.909 192.136 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R17 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value 3.3k (at -0.112 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(R17-Pad1)"))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 218.313 192.024 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R18 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value 100k (at -0.254 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 E+))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 /HT_U2B))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 294.513 185.024 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R19 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value 100k (at 0 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 F+))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 /HT_U1B))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 287.909 205.994)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R21 (at 0 -2.5) (layer F.SilkS))
    (fp_text value 2.2M (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C10-Pad2)"))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 199.898 165.212 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R24 (at 0.015 2.286 270) (layer F.SilkS))
    (fp_text value 220k (at 0.015 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 D+))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 41 /HT_U3A))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 152.781 195.834 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R25 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value 100k (at 0 -0.127 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 42 /HT_U3B))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 146.685 174.849 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R27 (at 0.03 2.286 270) (layer F.SilkS))
    (fp_text value 330k (at -0.097 -0.127 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C14-Pad1)"))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(K1-Pad4)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 140.589 181.864 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R28 (at 0 2.286 270) (layer F.SilkS))
    (fp_text value 82k (at -0.127 -0.127 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C14-Pad1)"))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(P7-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 131.445 197.739 90)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R29 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value 470k (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(R29-Pad1)"))
    (pad 2 thru_hole circle (at 7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C14-Pad2)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 118.491 165.989)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R30 (at 0 2.413) (layer F.SilkS))
    (fp_text value 100k (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 30 C+))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 /HT_U4A))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 115.062 205.359)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R31 (at 0 -2.5) (layer F.SilkS))
    (fp_text value 680R (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(R31-Pad1)"))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(R29-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 144.399 212.344)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R32 (at 0 -2.5) (layer F.SilkS))
    (fp_text value 33k (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(R29-Pad1)"))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 88.519 168.133 270)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R33 (at 0 -2.5 270) (layer F.SilkS))
    (fp_text value 100k (at -0.239 0 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 30 C+))
    (pad 2 thru_hole circle (at 7 0 270) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 /HT_U4B))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 91.694 204.216)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R34 (at 0 -2.5) (layer F.SilkS))
    (fp_text value 470k (at 0 0) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(C17-Pad1)"))
    (pad 2 thru_hole circle (at 7 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(R29-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:R_0.5W (layer F.Cu) (tedit 57BE122A)
    (at 106.299 131.445 90)
    (descr "Resistance 1/2W")
    (tags R)
    (autoplace_cost180 10)
    (fp_text reference R37 (at 0 -2.5 90) (layer F.SilkS))
    (fp_text value 100k (at 0 0 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(C19-Pad2)"))
    (pad 2 thru_hole circle (at 7 0 90) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(P12-Pad1)"))
    (model discret/resistor.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module A-wai_Turrets:TUBE_TRIODE (layer F.Cu) (tedit 57E5A344)
    (at 250 185)
    (descr Triode)
    (fp_text reference U2 (at -7.5 -17.5) (layer Cmts.User))
    (fp_text value ECC83 (at -7.5 -15) (layer Cmts.User))
    (pad 3 thru_hole circle (at -15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(R16-Pad1)") (clearance 0.5))
    (pad 2 thru_hole circle (at -19 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(R14-Pad2)") (clearance 0.5))
    (pad 8 thru_hole circle (at 15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(C7-Pad1)") (clearance 0.5))
    (pad "" np_thru_hole circle (at 0 0) (size 30 30) (drill 30) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -15.5 11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 /HT_U2B))
    (pad 6 thru_hole circle (at 15.5 -11) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 /HT_U2A))
    (pad 7 thru_hole circle (at 19 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS))
  )
  (module A-wai_Turrets:TUBE_PENTODE (layer F.Cu) (tedit 57E5A2CA)
    (at 130 125)
    (descr Pentode)
    (fp_text reference U5 (at -10 -17.5) (layer Cmts.User))
    (fp_text value 6V6 (at -10 -15) (layer Cmts.User))
    (pad 3 thru_hole circle (at 0 -19) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (pad 2 thru_hole circle (at -13.5 13.5) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(C19-Pad2)") (clearance 0.5))
    (pad 9 thru_hole circle (at 13.5 13.5) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 33 /HT_G2))
    (pad "" np_thru_hole circle (at 0 0) (size 30 30) (drill 30) (layers *.Cu *.Mask F.SilkS))
  )
  (module A-wai_Turrets:TUBE_PENTODE (layer F.Cu) (tedit 57E5A2D0)
    (at 200 125)
    (descr Pentode)
    (fp_text reference U6 (at -10 -17.5) (layer Cmts.User))
    (fp_text value 6V6 (at -10 -15) (layer Cmts.User))
    (pad 3 thru_hole circle (at 0 -19) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
    (pad 2 thru_hole circle (at -13.5 13.5) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(C20-Pad1)") (clearance 0.5))
    (pad 9 thru_hole circle (at 13.5 13.5) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 33 /HT_G2))
    (pad "" np_thru_hole circle (at 0 0) (size 30 30) (drill 30) (layers *.Cu *.Mask F.SilkS))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57E5A314)
    (at 269.494 123.19)
    (descr Turret)
    (tags DEV)
    (fp_text reference P15 (at 0 -4.5) (layer Cmts.User))
    (fp_text value "TO LD GND" (at 0 -3.81) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
  )
  (module A-wai_Turrets:TURRET (layer F.Cu) (tedit 57E59EDD)
    (at 75.692 204.978)
    (descr Turret)
    (tags DEV)
    (fp_text reference P20 (at 0 -4.191) (layer Cmts.User))
    (fp_text value "TO PA GND" (at 0 4.572) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 5.5 5.5) (drill 2.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (clearance 0.5))
  )
  (module Freetronics:SJ_OPEN (layer F.Cu) (tedit 54779663)
    (at 334.391 209.55 270)
    (descr "<b>Solder jumper</b>")
    (fp_text reference JP1 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value JUMPER (at 0 1.6 270) (layer Eco1.User) hide)
    (pad 1 smd rect (at -0.762 0 270) (size 1.1684 1.6002) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.762 0 270) (size 1.1684 1.6002) (layers F.Cu F.Mask)
      (net 45 Earth))
  )
  (gr_text "Evil Head v1.0\nA-wai Amplification" (at 172.212 149.479) (layer F.SilkS))
  (gr_text "LD GND" (at 152.781 206.629) (layer F.SilkS))
  (gr_text "LD EQ" (at 152.781 185.039) (layer F.SilkS))
  (gr_text "DEPTH GND" (at 146.685 199.644) (layer F.SilkS))
  (gr_text DEPTH (at 140.589 192.786) (layer F.SilkS))
  (gr_text "LD GAIN" (at 268.986 188.976) (layer F.SilkS))
  (gr_text "CLN VOL" (at 300.99 188.976) (layer F.SilkS))
  (gr_text "CLN GND" (at 291.211 169.291) (layer F.SilkS))
  (gr_text "CLN EQ" (at 291.084 147.32) (layer F.SilkS))
  (gr_text "LD GAIN" (at 259.969 119.38) (layer F.SilkS))
  (gr_text "C11  1n" (at 200.66 200.406 90) (layer F.SilkS))
  (gr_text "C3  1µ" (at 345.059 201.803 90) (layer F.SilkS))
  (gr_text "C7  1µ" (at 275.336 213.868) (layer F.SilkS))
  (gr_text "C12  1µ" (at 175.641 217.678) (layer F.SilkS))
  (gr_text MSTR- (at 75.692 199.263) (layer F.SilkS))
  (gr_line (start 347 220) (end 350 217) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 70 217) (end 73 220) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 70 103) (end 73 100) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 347 147) (end 350 150) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 272 100) (end 275 103) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 275 130) (end 285 140) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 302 147) (end 347 147) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 295 140) (end 302 147) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 285 140) (end 295 140) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 275 103) (end 275 130) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 70 103) (end 70 217) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 272 100) (end 73 100) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 350 217) (end 350 150) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 73 220) (end 347 220) (layer Edge.Cuts) (width 0.1))
  (zone (net 45) (net_name Earth) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.8))
    (min_thickness 0.5)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 354.253676 96.647) (xy 352.729676 221.996) (xy 63.804676 225.933) (xy 61.772676 96.647)
      )
    )
  )
  (zone (net 45) (net_name Earth) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.8))
    (min_thickness 0.5)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 58.674 90.678) (xy 361.569 94.615) (xy 357.124 225.298) (xy 53.848 231.902) (xy 56.515 91.313)
      )
    )
  )
)
